{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":1,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":61,"n_cols":12,"rows_kept":61,"cut":false,"hidden":false,"merged":[]}
[]
[null,"L103 MSL for Farmall 110U, 120U","L103 for Farmall Medium Utility U","L103 MSL for Farmall 90C-120C","L103 for Farmall 100A Series","L103 for Maxxum series","L103 for Vestrum series","L104","L105","L116","L108","L117"]
["Self-Levelling Feature"]
["Self-Levelling ","Mechanical","Non","Mechanical","Non","Non",null,"Mechanical","Mechanical","Mechanical","Mechanical","Mechanical"]
["Tractor Compatibility"]
["Matching Tractor Model Or Series, First ","Farmall 110U, 120U Tier 4B","Farmall 110U, 120U","Farmall 90C to 120C, Tier 4B","Farmall 110A, 120A, 130A, 140A","Maxxum 115 to 150 2WD Tier 4B",null,"Farmall 110A to 140A Tier 4B","Maxxum 115 to 150 Tier 4B","Puma 150-165 Short Wheel Base","Magnum 180-240","Puma 185-240 Long Wheel Base"]
["Matching Tractor Model Or Series, Second "]
["Matching Tractor Model Or Series, Third "]
["Tractor Tires Listed In Loader Specification "]
["Lift Capacities"]
["Lift Capacity To Maximum Height, At Pivot Pin lb","3064  [1390]","3814  [1730]","2866  [1300]","3373  [1530]","3836  [1740]",null,"3395  [1540]","4542  [2060]","5225  [2370]","5952  [2700]","5335  [2420]"]
["5.1.1 Lift Capacity To Maximum Height, At Bucket Pivot Pin lb"]
["Lift Capacity To Max. Height, 800mm (31.5in) Forward Of Pivot Pin lb","3461  [1570]","2359  [1070]","3241  [1470]","2094  [950]","2381  [1080]",null,"3814  [1730]","5203  [2360]","5578  [2530]","6151  [2790]","5622  [2550]"]
["5.1.2 Lift Capacity To Max. Height, 31.5\" (800 Mm) Forward Of Bucket Pivot Pin lb"]
["Lift Capacity To Max. Height, 500mm (19.7in) Forward Of Pivot Pin lb"]
["Lift Capacity To 1.5m (59in) at Pivot Pin lb","3439  [1560]","4233  [1920]","3219  [1460]","3770  [1710]","4277  [1940]",null,"3836  [1740]","5490  [2490]","6063  [2750]","7760  [3520]","6283  [2850]"]
["5.1.3 Lift Capacity To 59\" (1.5 M) Height, At Bucket Pivot Pin lb"]
["Lift Capacity To 1.5m (59in) Height, 800mm (31.5in) Forward Of Pivot Pin lb","3505  [1590]","3131  [1420]","3285  [1490]","2778  [1260]","3175  [1440]",null,"3858  [1750]","5512  [2500]","6107  [2770]","6680  [3030]","6349  [2880]"]
["5.1.4 Lift Capacity To 59\" (1.5 M) Height, 31.5\" (800 Mm) Forward Of Pivot Pin lb"]
["Lift Height Dimensions, Fully Raised"]
["Max Lift Height To Bucket Pivot Pin in","144  [3660]","144  [3660]","141  [3580]","145  [3680]","143  [3640]",null,"151  [3840]","162  [4120]","167  [4230]","174  [4410]","180  [4580]"]
["4.1.1 Maximum Lift Height To Bucket Pivot Pin in"]
["Max Lift Height Under Level Bucket in","132  [3350]","132  [3350]","129  [3270]","133  [3370]","131  [3330]",null,"139  [3530]","150  [3810]","154  [3920]","162  [4110]","168  [4270]"]
["4.1.2 Maximum Lift Height Under Level Bucket in"]
["Max Dump Clearance in","106  [2690]","106  [2690]","103  [2610]","107  [2710]","105  [2670]",null,"113  [2870]","124  [3150]","129  [3270]","136  [3450]","143  [3620]"]
["4.1.3 Clearance With Bucket Dumped 45 Degrees, Lowest Point Of Cutting Edge in"]
["Boom Lift Breakout Force"]
["Boom Breakout Force, At Pivot Pin, Bucket At Ground lbf","4057  [18]","4916  [21.9]","3792  [16.9]","4387  [19.5]","4982  [22.2]",null,"4409  [19.6]","6437  [28.6]","6878  [30.6]","9171  [40.8]","7121  [31.7]"]
["5.1.5 Boom Breakout Force, At Pivot Pin, Bucket At Ground, Lbs (kg) (kiloNewtons) "]
["Boom Breakout Force, 800mm (31.5in) Forward Of Pivot Pin At Ground lbf","3660  [16.3]","3395  [15.1]","3417  [15.2]","3020  [13.4]","3439  [15.3]",null,"3968  [17.65]","5975  [26.6]","6415  [28.5]","8620  [38.3]","6768  [30.1]"]
["5.1.6 Boom Breakout Force, 31.5\" (800 Mm) Forward Of Bucket Pivot Pin At Ground, Lbs (kg) (kiloNewtons) "]
["Bucket Rollback Force"]
["Bucket Rollback Force At Max. Height, 800mm (31.5in) Forward Of Pivot Pin lbf","3263  [14.5]","3064  [13.6]","3064  [13.6]","2734  [12.2]","3109  [13.8]",null,"4167  [18.5]","5357  [23.8]","6460  [28.7]","6768  [30.1]","6217  [27.7]"]
["5.1.7 Bucket Rollback Force At Max. Height, 31.5\" (800 Mm) Forward Of Pivot Pin, Lbs (kg) (kiloNewtons) "]
["Bucket Rollback Force At 1.5M (59in) Height, 800mm (31.5in) Forward Of Pivot Pin lbf"]
["5.1.8 Bucket Rollback Force At 59\" (1.5 M) Height, 31.5\" (800 Mm) Forward Of Pivot Pin, Lbs (kg) (kiloNewtons) "]
["Bucket Rollback Force At Ground, 800mm (31.5in) Forward Of Pivot Pin lbf","5357  [23.8]","5445  [24.2]","5004  [22.3]","4828  [21.5]","5490  [24.4]",null,"6680  [29.7]","8841  [39.3]","10274  [45.7]","10714  [47.7]","10406  [46.3]"]
["5.1.9 Bucket Rollback Force At Ground, 31.5\" (800 Mm) Forward Of Pivot Pin, Lbs (kg) (kiloNewtons) "]
["Horizontal Reach Distance"]
["Dump Reach At Maximum Lift Height in","37  [940]","37  [940]","39  [980]","47  [1200]","35.4  [900]",null,"38.2  [970]","28  [710]","38  [960]",null,"36  [920]"]
["4.1.4 Reach At Maximum Lift Height, Bucket Cutting Edge To Tractor Front, Bucket Dump At 45 Degrees in"]
["Ground Level Reach in","91  [2300]","91  [2300]","95  [2410]","88  [2240]","84  [2130]",null,"94.5  [2400]","99  [2520]","107  [2730]","120  [3050]","115  [2910]"]
["4.1.6 Reach With Bucket On Ground, Level, From Centerline Of Front Wheels To Bucket Cutting Edge in"]
["Dump And Rollback Angles"]
["Max Dump Angle, Loader Raised °",60,60,60,62,60,null,62,56,58,49,54]
["4.1.5 Maximum Dump Angle, Loader Fully Raised °"]
["Max Rollback Angle, Bucket At Ground °",43,43,46,42,44,null,45,47,48,65,50]
["4.1.7 Maximum Rollback Angle, Bucket At Ground °"]
["Digging Depth"]
["Digging Depth in","2.4  [60]","2.4  [60]","5.5  [140]","2  [50]","3.1  [80]",null,"5  [130]","3.9  [100]","7.5  [190]",null,"7.1  [180]"]
["4.1.8 Digging Depth, From Ground Line To Bottom Of Bucket With Cutting Edge Horizontal in"]
["Weight"]
["Weight lb"]
["Couplers For Buckets And Attachments"]
["First Coupler Type Available ","Skid-Steer style","Skid-Steer style","Skid-Steer style","Skid-Steer style","Skid-Steer style",null,"Skid-Steer style","Euro style only","Euro style","Euro style","Euro style"]
["Second Coupler Type Available ","Euro style","Euro style","Euro style","Euro style","Euro style",null,"Euro style"]
["Other Coupler Type Available "]
["Hydraulic Function, Ride And Detachable Features"]
["Third Function Valve Available ","Optional","Optional","Optional","Optional","No",null,"Optional","Optional","Optional","Optional","Optional"]
["Cushioned Hydraulic Ride Control ","Optional","Optional","Optional","Optional",null,null,"Optional","Optional","Standard","Standard","Standard"]
["Loader Quick-attach-detach From Tractor ","Standard","Standard","Standard","Standard","Standard",null,"Standard","Standard","Standard","Standard","Standard"]