{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":1,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":61,"n_cols":4,"rows_kept":61,"cut":false,"hidden":false,"merged":[]}
[]
[null,"L340A","L350A","L360A"]
["Self-Levelling Feature"]
["Self-Levelling ","Non","Non","Non"]
["Tractor Compatibility"]
["Matching Tractor Model Or Series, First ","Farmall 35A, 40A","Farmall 45C CVT, 55C CVT","Farmall 45C, 55C"]
["Matching Tractor Model Or Series, Second "]
["Matching Tractor Model Or Series, Third "]
["Tractor Tires Listed In Loader Specification ","25x8.50-14, R4 front; 43x16.0-20, R4 rear","8x16 front; 14.9x24, R1 rear","12-16.5 front; 17.5L-24, R4 rear"]
["Lift Capacities"]
["Lift Capacity To Maximum Height, At Pivot Pin lb","1259  [571]","2063  [936]","2677  [1214]"]
["5.1.1 Lift Capacity To Maximum Height, At Bucket Pivot Pin lb"]
["Lift Capacity To Max. Height, 800mm (31.5in) Forward Of Pivot Pin lb"]
["5.1.2 Lift Capacity To Max. Height, 31.5\" (800 Mm) Forward Of Bucket Pivot Pin lb"]
["Lift Capacity To Max. Height, 500mm (19.7in) Forward Of Pivot Pin lb","882  [400]","1760  [798]","1650  [748]"]
["Lift Capacity To 1.5m (59in) at Pivot Pin lb","1607  [729]"]
["5.1.3 Lift Capacity To 59\" (1.5 M) Height, At Bucket Pivot Pin lb"]
["Lift Capacity To 1.5m (59in) Height, 800mm (31.5in) Forward Of Pivot Pin lb","1191  [540] at 19.7\" (500) ahead of pin"]
["5.1.4 Lift Capacity To 59\" (1.5 M) Height, 31.5\" (800 Mm) Forward Of Pivot Pin lb"]
["Lift Height Dimensions, Fully Raised"]
["Max Lift Height To Bucket Pivot Pin in","92  [2337]","106.5  [2700]","108  [2743]"]
["4.1.1 Maximum Lift Height To Bucket Pivot Pin in"]
["Max Lift Height Under Level Bucket in","84  [2134]","99  [2510]","101.5  [2578]"]
["4.1.2 Maximum Lift Height Under Level Bucket in"]
["Max Dump Clearance in","64  [1626]","73.4  [1990]","82  [2083]"]
["4.1.3 Clearance With Bucket Dumped 45 Degrees, Lowest Point Of Cutting Edge in"]
["Boom Lift Breakout Force"]
["Boom Breakout Force, At Pivot Pin, Bucket At Ground lbf","2719  [12.1]","3465  [15.4]","4504  [20]"]
["5.1.5 Boom Breakout Force, At Pivot Pin, Bucket At Ground, Lbs (kg) (kiloNewtons) "]
["Boom Breakout Force, 800mm (31.5in) Forward Of Pivot Pin At Ground lbf","1913  [8.5] at 19.7\" (500) ahead of pin"]
["5.1.6 Boom Breakout Force, 31.5\" (800 Mm) Forward Of Bucket Pivot Pin At Ground, Lbs (kg) (kiloNewtons) "]
["Bucket Rollback Force"]
["Bucket Rollback Force At Max. Height, 800mm (31.5in) Forward Of Pivot Pin lbf"]
["5.1.7 Bucket Rollback Force At Max. Height, 31.5\" (800 Mm) Forward Of Pivot Pin, Lbs (kg) (kiloNewtons) "]
["Bucket Rollback Force At 1.5M (59in) Height, 800mm (31.5in) Forward Of Pivot Pin lbf"]
["5.1.8 Bucket Rollback Force At 59\" (1.5 M) Height, 31.5\" (800 Mm) Forward Of Pivot Pin, Lbs (kg) (kiloNewtons) "]
["Bucket Rollback Force At Ground, 800mm (31.5in) Forward Of Pivot Pin lbf",null,"3402  [15.1] at 19.7\" (500 mm) ahead of pin","3757  [16.7] at 19.7\" (500 mm) ahead of pin"]
["5.1.9 Bucket Rollback Force At Ground, 31.5\" (800 Mm) Forward Of Pivot Pin, Lbs (kg) (kiloNewtons) "]
["Horizontal Reach Distance"]
["Dump Reach At Maximum Lift Height in","42  [1067]","31.3  [792]","46.3  [1175]"]
["4.1.4 Reach At Maximum Lift Height, Bucket Cutting Edge To Tractor Front, Bucket Dump At 45 Degrees in"]
["Ground Level Reach in","76  [1930]","73  [1855]","86.2  [2189]"]
["4.1.6 Reach With Bucket On Ground, Level, From Centerline Of Front Wheels To Bucket Cutting Edge in"]
["Dump And Rollback Angles"]
["Max Dump Angle, Loader Raised °",48,50,59]
["4.1.5 Maximum Dump Angle, Loader Fully Raised °"]
["Max Rollback Angle, Bucket At Ground °",28,32,35]
["4.1.7 Maximum Rollback Angle, Bucket At Ground °"]
["Digging Depth"]
["Digging Depth in","5  [127]","3.9  [100]","9.3  [235]"]
["4.1.8 Digging Depth, From Ground Line To Bottom Of Bucket With Cutting Edge Horizontal in"]
["Weight"]
["Weight lb"]
["Couplers For Buckets And Attachments"]
["First Coupler Type Available ","Skid-steer style","Skid-steer style","Skid-steer style"]
["Second Coupler Type Available "]
["Other Coupler Type Available ","No","No","No"]
["Hydraulic Function, Ride And Detachable Features"]
["Third Function Valve Available ","No","No","No"]
["Cushioned Hydraulic Ride Control ","No","No","No"]
["Loader Quick-attach-detach From Tractor ","Standard","Standard","Standard"]