{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":1,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":48,"n_cols":7,"rows_kept":48,"cut":false,"hidden":false,"merged":[]}
[]
[null,"DC105","DC125","DC135","DC165","DC93","DC103"]
["Tongue"]
["Tongue Type ","Side-Pull, curved tongue","Side-Pull, curved tongue","Side-Pull, curved tongue","Side-Pull, curved tongue","Side-Pull, straight tongue","Side-Pull, curved tongue"]
["Cutter Bar"]
["Cutting Width ft-in","10ft 1in","11ft 7in","13ft 1in","16ft 5in","9ft 2in","10ft 4in"]
["Cutting Height - in (mm) ",{"$nulls":5},"1.0 to 2.7 (24 to 68) std.; 2.3 to 4.5 (58 to 115) opt."]
["Cutter Bar Tilt Angle °","2","2","2","2","2","2"]
["Cutter Bar Lubrication ","Sealed independent disc modules","Sealed independent disc modules","Sealed independent disc modules","Sealed independent disc modules","Sealed independent disc modules","Sealed independent disc modules"]
["Discs"]
["Number Of Discs ","6","7","8","10","7","8"]
["Number Of Knives Per Disc ","2","2","2","2","2","2"]
["Disc Speed rpm","2250","2250","2250","2250","3000","3000"]
["Disc Drive Components ","Shafts w/bevel gears","Shafts w/bevel gears","Shafts w/bevel gears","Shafts w/bevel gears","Shafts w/bevel gears","Shafts w/bevel gears"]
["Header"]
["Flotation ","Up & back, adjustable springs","Up & back, adjustable springs","Up & back, adjustable springs","Up & back, adjustable springs","Up & back, adjustable springs","Up & back, adjustable springs"]
["Conditioner"]
["Conditioner Type ","Rolls","Rolls","Roll or Flail","Rolls","Roll or Flail","Rolls or Tines"]
["Conditioner Drive ","4 HB V-belt & enclosed gears","4 HB V-belt & enclosed gears","4 HB v-belt; rolls also have enclosed gears","4 HB V-belt & enclosed gears","4 HB v-belt; rolls also have enclosed gears","4 HB v-belt; rolls also have enclosed gears"]
["Roll Conditioner"]
["Roll Length in","90","102","125","125","90","102"]
["Roll Diameter in","10.4","10.4","10.4","10.4","10.4","10.4"]
["Roll Speed rpm","640","760","760","760","647","647"]
["Roll Material ","Rubber","Rubber","Rubber","Rubber","Rubber","Rubber"]
["Optional Roll Material ",null,"Steel","Steel","Steel",null,"Steel"]
["Roll Surface Pattern ","Chevron intermeshing","Chevron intermeshing","Chevron intermeshing","Chevron intermeshing","Chevron intermeshing","Chevron intermeshing"]
["Flail Conditioner"]
["Rotor Length in","90","102","125",null,"90","102"]
["Rotor Diameter in","22","22","10.4",null,"22","22"]
["Number Of Flails ","90","100","120",null,"90","100"]
["Flail Shape ","Tapered","Tapered","Tapered",null,"Tapered","Tapered"]
["Tractor Requirements"]
["Min PTO Power Required hp","80","85","90","100","65","80"]
["PTO Rated Speed rpm","540","1000","1000","1000","540","540"]
["Hookup To Tractor Drawbar ","Category 2 / 3","Category 2 / 3","Category 2 / 3","Category 2 / 3","Category 2","Category 2"]
["Hookup To Tractor Hitch Lift Arms ","Swivel hitch option","Swivel hitch option","Swivel hitch option","Swivel hitch option",null,"Swivel hitch option"]
["Tractor Hitch Size ","Category 3","Category 3","Category 3","Category 3",null,"2-point hitch Category 2, 3N or 3"]
["Hydraulic Relief Pressure psi","1500","1500","1500","1500","1500","1500"]
["Dimensions"]
["Transport Width ft-in","10ft 1in","11ft 7in","13ft 1in","16ft 5in","9ft 11in","11ft 3in"]
["Transport Length ft-in","23ft 7in","27ft 5in","27ft 5in","32ft","17ft 7in","17ft 7in"]
["Transport Height ft-in","6ft 7in","6ft 7in","6ft 7in","6ft 7in","5ft 8in","5ft 3in"]
["Ground Clearance in","16.2","16.2","16.2","16.2","17","17"]
["Weight"]
["Weight With Roll Conditioner lb","5760","5880","6255","6980","3740","4160"]
["Weight With Flail Conditioner lb","5660","5760","6147",null,"3690","4100"]
["Tires"]
["Tire Size ","12.5L-15.8","12.5L-15.8","12.5L-15.8","12.5L-15.8","9.5Lx14L, 6PR","9.5Lx14L w/flail tines; 11Lx15L w/rolls"]