{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":1,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":44,"n_cols":5,"rows_kept":44,"cut":false,"hidden":false,"merged":[]}
[]
[null,"Tiger-Mate 255 Field Cultivator","Tiger-Mate 255 Double-Fold","Vibra-Tine 265 S-Tine Field Cultivator","Vibra-Tine S-Tine Field Cultivator, Double-Fold"]
["Dimensions And Weights"]
["Min Working Width ft-in","22ft 2in","37ft 5in","26ft 6in","36ft 6in"]
["Max Working Width ft-in","35ft 2in","60ft 1in","32ft 6in","48ft 6in"]
["Min Transport Width ft-in","14ft 11in","15ft 7in","16ft 4in","18ft 7in"]
["Max Transport Width ft-in","17ft","19ft","16ft 4in","18ft 7in"]
["Min Transport Height ft-in","10ft 2in","12ft 3in","11ft 3in","11ft 3in"]
["Max Transport Height ft-in","14ft 2in","15ft 6in","14ft","14ft"]
["Min Total Weight lb",8440,15725,12100,14100]
["Max Total Weight lb",10440,21860,13800,23300]
["Sizes Available ",5,6,4,6]
["Hitch And Frame"]
["Frame Configuration ","3 Section, Folding","5 Section, Folding","3 Section, Folding","5 Section, Folding"]
["Connection To Tractor ","Pull-Type, Category 3 or 4 drawbar","Pull-Type, Category 4 or 5 drawbar","Pull-Type, Category 2 or 3 drawbar","Pull-Type, Category 4 drawbar"]
["Pull-type Hitch System ","Constant level","Constant level or Floating","Constant level","Constant level"]
["Underframe Clearance in",25,25,24,24]
["Number Of Ranks ",5,5,6,6]
["Depth Control ","Electric - AFS Soil Command Hydraulic single point","Electric - AFS Soil Command Hydraulic single point","Hydraulic single point","Hydraulic single point"]
["Shanks"]
["Max Shank Tillage Depth in",6,6,4,4]
["Min Number Of Shanks ",41,69,78,106]
["Max Number Of Shanks ",65,111,96,144]
["Shank Spacing "]
["Shank Spacing - in (mm) ","6.5 (165)","6.5 (165)","12 (305)","4 (102)"]
["Shank Load "]
["Min Standard Trip Load lb",180,180,110,110]
["Max Standard Trip Load lb",180,180,110,110]
["Min Optional Trip Load lb",null,null,160,160]
["Max Optional Trip Load lb",null,null,160,160]
["Shank Trip Clearance in",14,14]
["Wheels And Axles"]
["Center Frame Tire Size ","280/70 R15","380/60 R16.5","280/70 R15","340/60 R16.5"]
["Wing Frame Tire Size ","280/70 R15","280/70 R15","280/70 R15","280/70 R15"]
["Transport Wheel Mounting ","Walking tandem","Walking tandem","Walking tandem","Walking tandem"]
["Gauge Wheel Size ","5.90x15 non-pivot","5.90x15 non-pivot"]
["Tractor Power Requirement"]
["Min Required Power hp/ft",5,5,5,5]
["Max Required Power hp/ft",10,10,10,10]
["Optional Attachments"]
["Coil Tine Harrow - Number Of Tine Bars ","2-bar or 4-bar Tiger-Tine","2-bar or 4-bar Tiger-Tine",3,3]
["Crumbler Or Basket Reel ","Mounted behind harrow, or trailing","Mounted behind harrow, or trailing"]
["Spike Harrow - Number Of Tine Bars ","3-bar","3-bar"]
["Rear Hitch For Trailing Equipment ","Optional","Optional","Optional","Optional"]