{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":1,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":61,"n_cols":8,"rows_kept":61,"cut":false,"hidden":false,"merged":[]}
[]
[null,"Steiger 425","Steiger 475","Steiger 525","Steiger 555","Steiger 595","Steiger 645","Steiger 715"]
["Description"]
["Classification Horsepower ",425,"475 HP",525,555,595,645,715]
["Drive Type ","Wheeled/Rowtrac","Wheeled/Rowtrac/Quadtrac Tractor","Wheeled/Rowtrac/Quadtrac Tractor","Wheeled/Quadtrac","Wheeled/Quadtrac","Wheeled/Quadtrac","Quadtrac"]
["Drive Configuration ",{"$nulls":4},"4WD","4WD"]
["Application "]
["Engine Performance"]
["Rated Engine Power hp","425 HP","475 HP",525,"555 HP",595,645,715]
["Max Power (No Boost) hp","467 HP","522 HP","578 HP","614 HP",656,699,778]
["Max Torque lbf/ft"]
["Electric Drivetrain Performance"]
["Type "]
["Phase "]
["Power hp"]
["Battery Type "]
["Voltage V"]
["Capacity Ah"]
["Power Take Off (PTO)"]
["Rear PTO "]
["PTO Power hp","409 HP","462 HP","516 HP","537 HP",537,537]
["540rpm "]
["540 Available? "]
["540E Available? "]
["1000rpm "]
["1000 Available? ","Optional","Optional","Optional",null,"Optional","Optional","Optional"]
["1000E Available? "]
["Front PTO "]
["Engine"]
["Make ","FPT","FPT","FPT",null,"FPT","FPT","FPT"]
["Model ","Cursor 13","Cursor 13","Cursor 13",null,"Cursor 13","Cursor 13","Cursor 16"]
["Electrical System"]
["Alternator ","12V 240 amp / 12V 330 amp","12V 240 amp / 12V 330 amp","12V 240 amp / 12V 330 amp"]
["Transmission Configuration"]
["Type ","Powershift","Powershift","Powershift","PowerDrive","PowerDrive","PowerDrive","PowerDrive"]
["Forward Speeds ",16,16,16,null,16,16,16]
["Reverse Speeds ",2,null,2,null,null,null,2]
["Max Speed Forward - mph (kph) ",25,25,25,null,25,25,26.5]
["Hydraulic System"]
["Standard Pump Flow gallon (US)/min","42 gpm",null,"42 gpm",null,42,42,"57 [High Capacity Hydraulic Pump]"]
["Standard Pump Pressure psi"]
["Remote Valves ",{"$nulls":6},"4 std; up to 8 total"]
["3-Point Hitch"]
["3-Point Hitch Category ","4N","4N","4N","Cat. 4N","Category 4N","Category 4N","Category 4N"]
["Standard Capacity 24 Inches Behind Pin lb",{"$nulls":6},"22250 (10095)"]
["Standard Capacity At Pin lb"]
["Max Lift Capacity lb","21,903 [9 934] / 21,903  [9 934] / N/A",null,"21,903 lb. (9 934 kg)","22,750 lb. (10 319 kg)",null,null,"22250 (10095)"]
["Dimensions"]
["Wheelbase in",148,"148 in.",154,null,null,154,"154 [3912]"]
["Length in"]
["Height Over Cab in"]
["Height Over ROPS in"]
["Overall Width in","120 in.","120 in.","120 in.",null,"120/88(Quadtrac)",120]
["Weight"]
["Unladen Weight lb",{"$nulls":6},"72,000"]
["Weight, Total Allowable lb","40,800  [18 507] / 56,000 [25 401] Wheeled","40,800 [18 507] / 56,000 [25 401] Wheeled","53,700 lb.\n[23 358 kg] / 67,000 lb.\n[30 390 kg](Quadtrac)","55,200 \n[25 038]/ 67,000\n[30 390 kg)]Quadtrac","56,800\n[25 764]/ 67,000\n[30 390 kg] Quadtrac\nQuadtrac","56,800 \n[25 764] / 67,000\n[30 390]\nQuadtrac","61200 [27760]"]
["Weight, Total Allowable To 40km/h lb",null,49500]
["Weight, Total Allowable To 50km/h lb",null,null,56000]
["Weight, Total Allowable To 60km/h lb"]
["Tire / Track Size"]
["Tracks "]