{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":1,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":51,"n_cols":4,"rows_kept":51,"cut":false,"hidden":false,"merged":[]}
[]
[null,"Axial-Flow 7150","Axial-Flow 6150","Axial-Flow 5150"]
["Headers"]
["Case IH  fixed/variable knife headers (2030/3050 range), draper headers (3152 range), flexheaders (3020 range) working widths (m): ","4.9 / 5.5 / 6.1 / 6.7 / 7.6 / 8.5 / 9.1","4.9 / 5.5 / 6.1 / 6.7 / 7.6 / 8.5","4.9 / 5.5 / 6.1 / 6.7"]
["Corn header 4400 range rigid / foldable ","6 & 8 row chopping corn heads","6 & 8 row chopping corn heads","6 & 8 row chopping corn heads"]
["Pickup headers 3016 range working width (m): ","3.7 / 4.6","3.7 / 4.6","3.7 / 4.6"]
["Threshing / separating"]
["Rotor drive type ","Variable belt with 3-speed transmission","Variable belt with 3-speed transmission","Variable belt with 3-speed transmission"]
["Rotor speed range (rpm) ","250 - 1.150 (3 ranges)","250 - 1.150 (3 ranges)","250 - 1.150 (3 ranges)"]
["Rotor diameter and length ( mm) ","762 / 2,794","762 / 2,794","762 / 2,794"]
["Total separation area (m2) ","2.78","2.78","2.78"]
["Threshing / separating modules wrap angle (°) ","156 / 133","156 / 133","156 / 133"]
["Number of threshing / separating modules ","6 / 3","6 / 3","6 / 3"]
["Cleaning system"]
["3 steps cleaning system ","Standard","Standard","Standard"]
["Cross Flow Cleaning System (for hillside harvesting) ","Option","Option","Option"]
["Cascade sieve ","-","-","-"]
["Cleaning shoe width (mm) ","1470","1470","1470"]
["Levelling capability (%) ","-","-","-"]
["Total sieve area under wind control (m2) ","5.5 / 5.4","5.5 / 5.4","5.5 / 5.4"]
["Cleaning fan"]
["Fan speed range (rpm) ","450 to 1,250","450 to 1,250","450 to 1,250"]
["Return system"]
["Tailings return type ","To rotor","To rotor","To rotor"]
["Grain tank / unloading"]
["In-cab control of grain tank covers ","Standard","Standard","Standard"]
["Grain tank capacity (l) ","Up to 10,570","Up to 10,570","Up to 8,800"]
["Unloading rate standard/high capacity (l/s) ","113","113","113"]
["Unloading auger effective length (m) ","6.4 / 7.3 / 7.7","6.4 / 7.3 / 7.7","6.4 / 7.3 / 7.7"]
["Straw chopper & spreader"]
["Straw chopper / beater ","Integral flail-type straw chopper","Integral flail-type straw chopper","Integral flail-type straw chopper"]
["Number of knives: chopper / counterbar ","54 / 32","54 / 32","54 / 32"]
["Spreader type ","dual horizontal spreaders and foldable windrow chute","dual horizontal spreaders and foldable windrow chute","dual horizontal spreaders and foldable windrow chute"]
["Engine"]
["Type / Capacity (cm3) ","6 cylinder, Turbo, aftercooler / 8.700","6 cylinder, Turbo, aftercooler / 8.700","6 cylinder, Turbo, aftercooler / 6.700"]
["Emission stage ","V","V","V"]
["Max. power HP (kW) ECE R120 at  rpm ","460 (338) @ 2000","400 (295) @ 2000","312 (230) @ 2000"]
["Fuel tank: diesel / urea (l) ","950 (166)","950 (166)","950 (166)"]
["Traction"]
["Transmission ","Hi / Lo Hydrostatic drive, 2 speed ranges in transmission","Hi / Lo Hydrostatic drive, 2 speed ranges in transmission","Hi / Lo Hydrostatic drive, 2 speed ranges in transmission"]
["Heavy duty adjustable steering axle ","Standard","Standard","Standard"]
["Final drive type ","Bull gear","Bull gear","Bull gear"]
["Powered rear axle ","Optional","Optional","Optional"]
["Differential lock ","-","-","-"]
["Operator lab"]
["Comfort cab ","Standard","Standard","Standard"]
["Luxury cab ","Optional","Optional","Optional"]
["Precision Technology"]
["Yield & Moisture monitor / mapping ","Optional","Optional","Optional"]
["Precision Farming ready and Guidance ready ","Optional","Optional","Optional"]
["Guidance ready ","-","-","-"]