{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":1,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":40,"n_cols":2,"rows_kept":40,"cut":false,"hidden":false,"merged":[]}
[]
["Technical Specifications","MAXXUM 150 CVXDRIVE"]
["ENGINE"]
["FPT - EU Stage V (Hi-eSCR2)<br class=\"t-last-br\" />","✓"]
["Rated power acc. ECE R120 [kW/hp]<br class=\"t-last-br\" />","110 / 150"]
["Maximum power acc. ECE R120 [kW/hp]<br class=\"t-last-br\" />","116 / 158"]
["Maximum power acc. ECE R120 with Boost [kW/hp]<br class=\"t-last-br\" />","129 / 175"]
["Number of cylinder / capacity [cm3]<br class=\"t-last-br\" />","6 / 6,728"]
["Max torque [Nm]<br class=\"t-last-br\" />","740 @ 1,500 rpm"]
["Torque rise [%]<br class=\"t-last-br\" />",40]
["<span style=\"background-color: #ffffff; text-align: left; letter-spacing: normal; color: #444444;\">Diesel / AdBlue capacity [litres]</span>","250 / 39"]
["TRANSMISSION"]
["<span style=\"background-color: #ffffff; text-align: left; letter-spacing: normal; color: #444444;\">CVXDrive - Continuously variable transmission 50 kph ECO</span><br class=\"t-last-br\" />\n<br class=\"t-last-br\" />","✓"]
["APM (Automatic Productivity Management), electrical parking brake<br class=\"t-last-br\" />","✓"]
["Dual clutch technology, \"Auto Hold\"-function<br class=\"t-last-br\" />","✓"]
["Advanced Trailer Brake (active transmission - trailer brake system)<br class=\"t-last-br\" />","✓"]
["HYDRAULICS"]
["Axial piston pump with load sensing<br class=\"t-last-br\" />","150 l/min"]
["Electrical rear remotes + Power Beyond<br class=\"t-last-br\" />",3]
["Electrical mid mounts",2]
["External control of 3rd rear SCV<br class=\"t-last-br\" />","✓"]
["PTO"]
["540E/1,000/1,000E @ 1,592/1,893/1.621 rpm<br class=\"t-last-br\" />","✓"]
["PTO-Management, Soft start, external control<br class=\"t-last-br\" />\n<br class=\"t-last-br\" />","✓"]
["REAR LINKAGE"]
["EDC with dynamic ride control - max. lift capacity 7,867 kg<br class=\"t-last-br\" />","✓"]
["Automatic slip control, external control<br class=\"t-last-br\" />","✓"]
["CONFIGURATION"]
["AFS Pro 700 Plus monitor with ISOBUS Cl. III<br class=\"t-last-br\" />","✓"]
["Front axle and cab suspension<br class=\"t-last-br\" />","✓"]
["Automatic air conditioning, leather steering wheel, 12 LED work lights<br class=\"t-last-br\" />","✓"]
["Front hitch (inlcuding FH-Management)<br class=\"t-last-br\" />\n<br class=\"t-last-br\" />","✓"]
["Headland management  HMC  II &amp; configurable remotes<br class=\"t-last-br\" />","✓"]
["AFS Connect AdvancedTelematics + Adaptive Steering Control (Fast steering)<br class=\"t-last-br\" />","✓"]
["AccuGuide + Accu Turn Pro<br class=\"t-last-br\" />","✓"]
["FRONT LOADER Case IH L4225T"]
["PCH-System - hydraulic self leveling,  FITLOCK2+ System&reg;- automatic hitching  incl. multi-connection,<br class=\"t-last-br\" />","✓"]
["SHOCK ELIMINATOR suspension, EURO implement carrier<br class=\"t-last-br\" />","✓"]
["4,15 m max. lift height @ implement pivot<br class=\"t-last-br\" />","✓"]
["2.615 kg max. payload 600 mm from implement pivot axis<br class=\"t-last-br\" />","✓"]