{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":1,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":36,"n_cols":2,"rows_kept":36,"cut":false,"hidden":false,"merged":[]}
[]
["Technical Specifications","OPTUM 340 CVXDRIVE"]
["ENGINE"]
["FPT - EU Stage V (Hi-eSCR2)<br class=\"t-last-br\" />","✓"]
["Rated power acc. ECE R120 [kW/hp]<br class=\"t-last-br\" />","250 / 340"]
["Maximum power acc. ECE R120 [kW/hp]<br class=\"t-last-br\" />","250 / 340"]
["Number of cylinder / capacity [cm3]<br class=\"t-last-br\" />","6 / 6,728"]
["Max torque [Nm]<br class=\"t-last-br\" />","1,398 @ 1,400 rpm"]
["Torque rise [%]<br class=\"t-last-br\" />",23]
["<span style=\"background-color: #ffffff; text-align: left; letter-spacing: normal; color: #444444;\">Diesel / AdBlue capacity [litres]</span>","630 / 96"]
["Fan<br class=\"t-last-br\" />","ECO Fan with engine brake function"]
["TRANSMISSION"]
["CVXDrive - Continuously variable transmission 50 kph ECO<br class=\"t-last-br\" />","✓"]
["APM (Automatic Productivity Management), electrical parking brake<br class=\"t-last-br\" />","✓"]
["Dual clutch technology, \"auto hold\"-function<br class=\"t-last-br\" />","✓"]
["Advanced Trailer Brake (active transmission - trailer brake system)<br class=\"t-last-br\" />","✓"]
["HYDRAULICS"]
["Axial piston pump with load sensing<br class=\"t-last-br\" />","220 l/min"]
["Electrical rear remotes + Power Beyond<br class=\"t-last-br\" />",5]
["Electrical mid mounts + Advanced Joystick<br class=\"t-last-br\" />\n<br class=\"t-last-br\" />",2]
["PTO"]
["540/540E/1,000/1,000E @ 1,871/1,598/1,853/1,583 rpm<br class=\"t-last-br\" />","✓"]
["PTO-Management, Soft start, external control<br class=\"t-last-br\" />\n<br class=\"t-last-br\" />","✓"]
["REAR LINKAGE"]
["EDC with dynamic ride control - max. lift capacity 11,058 kg<br class=\"t-last-br\" />\n<br class=\"t-last-br\" />","✓"]
["Automatic slip control, external control<br class=\"t-last-br\" />","✓"]
["CONFIGURATION"]
["AFS Pro 1200 monitor with ISOBUS Cl. III / TIM<br class=\"t-last-br\" />","✓"]
["Suspended front axle and semi-active suspended cab (optional)<br class=\"t-last-br\" />","✓"]
["Luxury cabin: leather equipment + active suspended driver seat<br class=\"t-last-br\" />","✓"]
["360&deg; LED working lights, front camera<br class=\"t-last-br\" />","✓"]
["Front hitch (including front hitch-Management)<br class=\"t-last-br\" />","✓"]
["Auto guidance System AccuGuide &amp; AccuTurn Pro (automatic turning)<br class=\"t-last-br\" />","✓"]
["Headland management HMC  II<br class=\"t-last-br\" />\n<br class=\"t-last-br\" />","✓"]
["AFS Connect Advanced Telematics, Adaptive Steering Control (Fast steering)<br class=\"t-last-br\" />","✓"]
["Baler automation through lidar sensor<br class=\"t-last-br\" />","✓"]