{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":1,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":37,"n_cols":2,"rows_kept":37,"cut":false,"hidden":false,"merged":[]}
[]
["Technical Specifications","LB436 HD"]
["BALE DIMENSIONS"]
["Width x height<br class=\"t-last-br\" />","120 x 90 cm"]
["Maximum lenght<br class=\"t-last-br\" />","300 cm​"]
["TRACTOR REQUIREMENTS"]
["Minimum PTO power [kW/hp]<br class=\"t-last-br\" />\n<br class=\"t-last-br\" />","184 / 250"]
["Hydraulic distribution<br class=\"t-last-br\" />","(single) 1"]
["Hydraulic distribution<br class=\"t-last-br\" />","(double)\t2"]
["PICK-UP"]
["Width<br class=\"t-last-br\" />\n<br class=\"t-last-br\" />","2,352 mm​"]
["Guard type Poly plastic pick-up<br class=\"t-last-br\" />","✓"]
["Guard wheels fixed or castering<br class=\"t-last-br\" />","✓"]
["FEEDING SYSTEM"]
["Type<br class=\"t-last-br\" />","Rotor"]
["Maximum number of knives<br class=\"t-last-br\" />",29]
["Knive activation in / out hydraulic<br class=\"t-last-br\" />","✓"]
["Knive protection Individual springs<br class=\"t-last-br\" />","✓"]
["PLUNGER"]
["Speed<br class=\"t-last-br\" />","48 strokes / min."]
["TYING SYSTEM"]
["Type<br class=\"t-last-br\" />","TwinePro – Double knotter"]
["Twine type TAMA SUPREME HD<br class=\"t-last-br\" />","✓"]
["Number of knotters<br class=\"t-last-br\" />",6]
["Knotter fans and type<br class=\"t-last-br\" />"," 3 electric fans​"]
["Knotter function alert<br class=\"t-last-br\" />","✓"]
["Twine bale capacity<br class=\"t-last-br\" />","36 twine XL spools"]
["TYRES"]
["Steered tandem axle large tyres<br class=\"t-last-br\" />","600/55 – 26.5​ ​"]
["BALER DIMENSIONS"]
["Width overall<br class=\"t-last-br\" />","3,000 mm​"]
["Weight<br class=\"t-last-br\" />","14,500 kg"]
["OTHER EQUIPMENT"]
["Baler Automation with Lidar Sensor<br class=\"t-last-br\" />","✓"]
["Automatic steering<br class=\"t-last-br\" />","✓"]
["Automatic tractor speed adjustment<br class=\"t-last-br\" />","✓"]
["Pro-active system<br class=\"t-last-br\" />","✓"]