{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":1,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":37,"n_cols":2,"rows_kept":37,"cut":false,"hidden":false,"merged":[]}
[]
["Technical Specifications","VESTRUM SERIES"]
["ENGINE"]
["FPT - EU Stage V (Hi-eSCR2) <br class=\"t-last-br\" />\n<br class=\"t-last-br\" />","✓"]
["Rated power acc. ECE R120 [kW/hp]<br class=\"t-last-br\" />","96 / 130"]
["Maximum power acc. ECE R120 [kW/hp]<br class=\"t-last-br\" />","103 / 140"]
["Number of cylinder / capacity [cm3]<br class=\"t-last-br\" />","4 / 4,500"]
["Max torque [Nm]<br class=\"t-last-br\" />","630 @ 1,300 rpm"]
["Torque rise [%]<br class=\"t-last-br\" />",41]
["<span style=\"background-color: #ffffff; text-align: left; letter-spacing: normal; color: #444444;\">Diesel / AdBlue capacity [litres]</span>","180 / 19"]
["TRANSMISSION"]
["ActiveDrive 8 - 24x24 gears, 8-speed Powershift with automatic functions, 40 kph<br class=\"t-last-br\" />","✓"]
["APM (Automatic Productivity Management), Smart Range Shift, Memory Shuttle<br class=\"t-last-br\" />","✓"]
["Dual clutch technology, Smooth Shift, Active Clutch II<br class=\"t-last-br\" />","✓"]
["HYDRAULICS"]
["Axial piston pump with load sensing<br class=\"t-last-br\" />","110 l/min"]
["Electrical rear remotes, low pressure return<br class=\"t-last-br\" />\n<br class=\"t-last-br\" />",4]
["Electrical mid mounts, advanced joystick (additional functions)<br class=\"t-last-br\" />\n<br class=\"t-last-br\" />\n<br class=\"t-last-br\" />",2]
["External fender controls<br class=\"t-last-br\" />\n<br class=\"t-last-br\" />\n<br class=\"t-last-br\" />","3rd remote, rear hitch and PTO"]
["PTO"]
["540/540E/1,000 @ 1,969/1,546/1,893 rpm<br class=\"t-last-br\" />","✓"]
["PTO-Management, Soft start, external control<br class=\"t-last-br\" />\n<br class=\"t-last-br\" />","✓"]
["REAR LINKAGE"]
["EDC with dynamic ride control - max. lift capacity 5,600 kg<br class=\"t-last-br\" />\n<br class=\"t-last-br\" />\n<br class=\"t-last-br\" />","✓"]
["Automatic slip control, external control<br class=\"t-last-br\" />\n<br class=\"t-last-br\" />\n<br class=\"t-last-br\" />","✓"]
["CONFIGURATION"]
["AFS Pro 700 Plus monitor with ISOBUS Cl. III<br class=\"t-last-br\" />\n<br class=\"t-last-br\" />\n<br class=\"t-last-br\" />","✓"]
["Front axle and cab suspension <br class=\"t-last-br\" />\n<br class=\"t-last-br\" />","✓"]
["Low roof cab with Panorama high visibility window<br class=\"t-last-br\" />","✓"]
["Automatic air conditioning, leather steering wheel, 14 LED work lights<br class=\"t-last-br\" />","✓"]
["Front hitch (inlcuding FH-Management)<br class=\"t-last-br\" />\n<br class=\"t-last-br\" />","✓"]
["Headland management HMC&nbsp; II &amp; configurable remotes<br class=\"t-last-br\" />\n<br class=\"t-last-br\" />","✓"]
["FRONT LOADER Case IH L4022U"]
["<span style=\"background-color: #ffffff; text-align: left; letter-spacing: normal; color: #444444;\">Mechanical self leveling, FITLOCK2+ System&reg;- automatic hitching incl. multi-connection</span>","✓"]
["SHOCK ELIMINATOR suspension, EURO implement carrier<br class=\"t-last-br\" />","✓"]
["3.95 m max. lift height<br class=\"t-last-br\" />","✓"]
["<span style=\"background-color: #ffffff; text-align: left; letter-spacing: normal; color: #444444;\"></span><span style=\"background-color: #ffffff; text-align: left; letter-spacing: normal; color: #444444;\">2.355 kg max. payload </span><span style=\"background-color: #ffffff; text-align: left; letter-spacing: normal; color: #444444;\">600 </span><span style=\"background-color: #ffffff; text-align: left; letter-spacing: normal; color: #444444;\">mm from implement pivot axis </span>","✓"]