{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":1,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":43,"n_cols":2,"rows_kept":43,"cut":false,"hidden":false,"merged":[]}
[]
["Technical Specifications","RB456 HD Pro "]
["BALE DIMENSIONS"]
["Bale diameter [cm]<br class=\"t-last-br\" />","90 / 165"]
["Width [cm]<br class=\"t-last-br\" />",120]
["TRACTOR REQUIREMENTS"]
["Minimum PTO power [kW/hp]<br class=\"t-last-br\" />\n<br class=\"t-last-br\" />","88 / 120"]
["Overall protection&nbsp;&nbsp;&nbsp; <br class=\"t-last-br\" />\n<br class=\"t-last-br\" />\n<br class=\"t-last-br\" />","Cut-Out Clutch"]
["PTO speed<br class=\"t-last-br\" />\n<br class=\"t-last-br\" />\n<br class=\"t-last-br\" />\n<br class=\"t-last-br\" />","1,000"]
["PICK-UP"]
["Width, effective (DIN 11220) [m]<br class=\"t-last-br\" />",2.3]
["Number of tine bars",5]
["Windguard type","Roller"]
["Pickup wheels","Gauge wheels (15/6.00 - 6)"]
["FEEDER & CROP CUTTER"]
["Type<br class=\"t-last-br\" />","Rotor „V“ shape"]
["Feeding system<br class=\"t-last-br\" />","Rotor Cutter 25 knives"]
["Top Assist Roll<br class=\"t-last-br\" />","✓"]
["Active Drop Floor<br class=\"t-last-br\" />","✓"]
["BALE FORMATION"]
["Type<br class=\"t-last-br\" />","Hydraulic"]
["Number of belts<br class=\"t-last-br\" />\n<br class=\"t-last-br\" />\n<br class=\"t-last-br\" />","4 x 273 mm endless"]
["Density control<br class=\"t-last-br\" />\n<br class=\"t-last-br\" />\n<br class=\"t-last-br\" />","In-cab control through monitor"]
["WRAPPING SYSTEM"]
["Net wrapping system","Duckbill net feeding"]
["Net storage","1 active + 2 spare"]
["Net coverage","Edge to edge"]
["MONITOR"]
["Baler control system","AFS Pro 700"]
["TYRES AND BRAKES"]
["Available sizes<br class=\"t-last-br\" />","500/55-20 or 620/40-22.5"]
["Brakes<br class=\"t-last-br\" />\n<br class=\"t-last-br\" />","Hydraulic or Pneumatic"]
["BALER DIMENSIONS"]
["Width on 500/55-20 tyres [mm]","2,742"]
["Width on 620/40-22.5 tyres [mm]<br class=\"t-last-br\" />\n<br class=\"t-last-br\" />","2,910"]
["Total length [mm]<br class=\"t-last-br\" />","4,865"]
["Total height [mm]<br class=\"t-last-br\" />\n<br class=\"t-last-br\" />","3,170"]
["Weight [kg]<br class=\"t-last-br\" />","3,500"]
["OTHER EQUIPMENT"]
["Automatic chain lubrication<br class=\"t-last-br\" />","✓"]
["Automatic chain greasing<br class=\"t-last-br\" />","Option"]
["LED under shield service lights<br class=\"t-last-br\" />","Option"]
["Beacon light<br class=\"t-last-br\" />","Option"]