{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":1,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":34,"n_cols":2,"rows_kept":34,"cut":false,"hidden":false,"merged":[]}
[]
["Technical Specifications","PUMA 260 CVXDRIVE"]
["ENGINE"]
["FPT - EU Stage V (Hi-eSCR2)<br class=\"t-last-br\" />","✓"]
["Rated power acc. ECE R120 [kW/hp]<br class=\"t-last-br\" />","191 / 260"]
["Maximum power acc. ECE R120 [kW/hp]<br class=\"t-last-br\" />","207 / 281"]
["<span style=\"background-color: #ffffff; text-align: left; letter-spacing: normal; color: #444444;\">Maximum power with Power Boost acc. ECE R120 [kW/hp]</span>","222 / 302"]
["Number of cylinder / capacity [cm3]<br class=\"t-last-br\" />","6 / 6,728"]
["Max torque [Nm]<br class=\"t-last-br\" />","1,249 @ 1,500 rpm"]
["Torque rise [%]<br class=\"t-last-br\" />",39]
["<span style=\"background-color: #ffffff; text-align: left; letter-spacing: normal; color: #444444;\">Diesel / AdBlue capacity [litres]</span>","470 / 54"]
["TRANSMISSION"]
["<span style=\"background-color: #ffffff; text-align: left; letter-spacing: normal; color: #444444;\">CVXDrive - Continuously variable transmission 50 kph ECO</span><br class=\"t-last-br\" />\n<br class=\"t-last-br\" />","✓"]
["APM (Automatic Productivity Management), electrical parking brake<br class=\"t-last-br\" />","✓"]
["Dual clutch technology, \"Auto Hold\"-function<br class=\"t-last-br\" />","✓"]
["Advanced Trailer Brake (active transmission - trailer brake system)<br class=\"t-last-br\" />","✓"]
["HYDRAULICS"]
["Axial piston pump with load sensing<br class=\"t-last-br\" />","170 l/min"]
["Electrical rear remotes + Power Beyond<br class=\"t-last-br\" />",4]
["2. Electrical mid mounts + Advanced joystick<br class=\"t-last-br\" />",2]
["PTO"]
["540/540E/1,000/1,000E @ 1,931/1,598/1,912/1,583 rpm<br class=\"t-last-br\" />","✓"]
["PTO-Management, Soft start, external control<br class=\"t-last-br\" />\n<br class=\"t-last-br\" />","✓"]
["REAR LINKAGE"]
["EDC with dynamic ride control - max. lift capacity 10,464 kg<br class=\"t-last-br\" />","✓"]
["Automatic slip control, external control<br class=\"t-last-br\" />","✓"]
["CONFIGURATION"]
["AFS Pro 1200 monitor with ISOBUS Cl. III / TIM<br class=\"t-last-br\" />","✓"]
["Active suspended front axle and cabin suspension<br class=\"t-last-br\" />","✓"]
["Automatic air conditioning, leather steering wheel, 360&deg; LED work lights<br class=\"t-last-br\" />","✓"]
["Front hitch (inlcuding FH-Management)<br class=\"t-last-br\" />\n<br class=\"t-last-br\" />","✓"]
["Auto guidance System AccuGuide &amp; AccuTurn Pro (automatic turning)<br class=\"t-last-br\" />","✓"]
["Headland management HMC  II<br class=\"t-last-br\" />","✓"]
["AFS Connect Advanced Telematics, Adaptive Steering Control (Fast steering)<br class=\"t-last-br\" />","✓"]