{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":1,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":25,"n_cols":2,"rows_kept":25,"cut":false,"hidden":false,"merged":[]}
[]
["Technical Specifications","FARMLIFT SERIES"]
["TELESCOPIC LOADER"]
["Max. lift capacity [kg]<br class=\"t-last-br\" />","4,200"]
["Max. lift height [m]<br class=\"t-last-br\" />",7]
["HYDRAULICS"]
["Piston pump flow [l/min]<br class=\"t-last-br\" />","140 / optional 160"]
["Hydraulic Oil tank [litres]<br class=\"t-last-br\" />",105]
["ENGINE FPT"]
["Rated power [kW/hp]<br class=\"t-last-br\" />","96 / 129"]
["Maximum power [kW/hp]<br class=\"t-last-br\" />","170 / 146"]
["TRANSMISSION "]
["6 x 3 Powershift (manual and auto shifting), 40 kph<br class=\"t-last-br\" />","✓"]
["CONFIGURATION SMART HYDRAULIC FEATURES"]
["Bucket shaking function<br class=\"t-last-br\" />\n<br class=\"t-last-br\" />","✓"]
["\"Back to position\" storage and automatic approach to the upper and lower arm and shovel positions<br class=\"t-last-br\" />","✓"]
["Engine speed management<br class=\"t-last-br\" />","✓"]
["Electro-hydraulic self-leveling<br class=\"t-last-br\" />","✓"]
["Adjustable aggressiveness of the shuttle behavior forward and reverse<br class=\"t-last-br\" />","✓"]
["Vertical lift<br class=\"t-last-br\" />","✓"]
["Adjustable boom response<br class=\"t-last-br\" />","✓"]
["Vibration dampening<br class=\"t-last-br\" />","✓"]
["7-inch display<br class=\"t-last-br\" />","✓"]
["Auto backup camera<br class=\"t-last-br\" />","✓"]
["Ergonomic joystick with the main functions<br class=\"t-last-br\" />","✓"]