{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":1,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":33,"n_cols":2,"rows_kept":33,"cut":false,"hidden":false,"merged":[]}
[]
["Technical Specifications","AXIAL-FLOW 7160"]
["ENGINE"]
["FPT &ndash; Cursor 9 - EU Stage V<br class=\"t-last-br\" />","✓"]
["Maximum power acc. ECE R120 [kW/hp]<br class=\"t-last-br\" />","338 / 460"]
["Number of cylinder / capacity [cm3]<br class=\"t-last-br\" />","6 / 8,700"]
["<span style=\"background-color: #ffffff; text-align: left; letter-spacing: normal; color: #444444;\">Diesel / AdBlue capacity [litres]</span>","950 / 166"]
["THRESHING / SEPARATING"]
["Rotor drive type<br class=\"t-last-br\" />","Variable belt with 3-speed transmission​"]
["Rotor speed range<br class=\"t-last-br\" />","250 - 1,150 rpm (3 ranges)​"]
["Rotor diameter and length<br class=\"t-last-br\" />","762 mm / 2,794 mm"]
["Total separation area<br class=\"t-last-br\" />"," 2.78 m2​"]
["Threshing / separating modules wrap angle<br class=\"t-last-br\" />","156° / 133°"]
["Number of threshing / separation modules<br class=\"t-last-br\" />","2026-06-03"]
["CLEANING SYSTEM"]
["3 steps cleaning system, optional Cross Flow cleaning system (for hillside harvesting)<br class=\"t-last-br\" />","✓"]
["Total sieve area under wind control - Fixed cleaning<br class=\"t-last-br\" />"," 5.52 m2​"]
["Total sieve area under wind control - Cross Flow cleaning<br class=\"t-last-br\" />\n<br class=\"t-last-br\" />","5.4 m2​"]
["RETURN SYSTEM"]
["Tailings return to rotor<br class=\"t-last-br\" />","✓"]
["GRAIN TANK / UNLOADING"]
["In-cab control of grain tank covers<br class=\"t-last-br\" />","✓"]
["Grain tank capacity<br class=\"t-last-br\" />","12,500 l​"]
["Unloading rate<br class=\"t-last-br\" />","113 l/s​"]
["Unloading auger effective length, measured from middle of combine to tip of unloading auger [m]<br class=\"t-last-br\" />","6.6 / 7.4 / 7.8​"]
["STRAW CHOPPER & SPREADER"]
["Integral flail-type straw chopper<br class=\"t-last-br\" />","✓"]
["Number of knives: chopper / counterbar<br class=\"t-last-br\" />","52 / 32"]
["Dual horizontal spreaders and foldable windrow chute<br class=\"t-last-br\" />","✓"]
["AUTOMATION"]
["AFS Harvest Command<sup>TM</sup><br class=\"t-last-br\" />","✓"]
["Harvesting strategies<br class=\"t-last-br\" />",3]
["Patented sieve pressure sensors and multi spectrum grain quality camera<br class=\"t-last-br\" />","✓"]