{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":1,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":38,"n_cols":2,"rows_kept":38,"cut":false,"hidden":false,"merged":[]}
[]
["Technical Specifications","FARMALL 100C"]
["ENGINE"]
["FPT - EU Stage V [Hi-eSCR2]<br class=\"t-last-br\" />","✓"]
["Rated power acc. ECE R120 [kW/hp]<br class=\"t-last-br\" />","74 / 100"]
["Number of cylinder / capacity [cm3]<br class=\"t-last-br\" />","4 / 3,600"]
["Max torque [Nm]<br class=\"t-last-br\" />","450 @ 1,300 rpm"]
["Torque rise [%]<br class=\"t-last-br\" />",47]
["<span style=\"background-color: #ffffff; text-align: left; letter-spacing: normal; color: #444444;\">Diesel / AdBlue capacity [litres]</span>","130 / 10"]
["TRANSMISSION"]
["ActiveDrive 2 - 24x24 gears, 2-speed Powershift, 40 kph ECO<br class=\"t-last-br\" />","✓"]
["Adjustable Powershuttle<br class=\"t-last-br\" />","✓"]
["Multicontroller gear lever incl. Powerclutch<br class=\"t-last-br\" />","✓"]
["HYDRAULICS"]
["Open Center pump 64 l/min + 36 l/min steering pump<br class=\"t-last-br\" />","✓"]
["Mechanical rear remote valves + diverter<br class=\"t-last-br\" />",3]
["Mid-mount valves with Advanced joystick<br class=\"t-last-br\" />",2]
["PTO"]
["540 / 540E / 1,000 @ 1,938 / 1,535 / 1,926 rpm<br class=\"t-last-br\" />","✓"]
["Hydraulic PTO<br class=\"t-last-br\" />","✓"]
["Soft start, external control<br class=\"t-last-br\" />","✓"]
["REAR LINKAGE"]
["EDC - max. lift capacity 4,400 kg,<br class=\"t-last-br\" />","✓"]
["External lift rams<br class=\"t-last-br\" />",2]
["External rear fender control<br class=\"t-last-br\" />","✓"]
["CONFIGURATION"]
["High visibility roof panel<br class=\"t-last-br\" />","✓"]
["Wide angle mirror<br class=\"t-last-br\" />","✓"]
["Air-conditioning system&nbsp;<br class=\"t-last-br\" />","✓"]
["Air suspended driver seat with armrest (15&deg; pivotable)<br class=\"t-last-br\" />","✓"]
["Working lights&nbsp;<br class=\"t-last-br\" />",6]
["Front linkage and front PTO<br class=\"t-last-br\" />","✓"]
["Air trailer brake system<br class=\"t-last-br\" />","✓"]
["FRONT LOADER CASE IH L3815A"]
["Mechanical self-levelling, FITLOCK2+ System&reg;  automatic hitching incl. multi-connection<br class=\"t-last-br\" />\n<br class=\"t-last-br\" />","✓"]
["SHOCK ELIMINATOR suspension, EURO implement carrier<br class=\"t-last-br\" />","✓"]
["3.85 m max. lift height @ implement pivot<br class=\"t-last-br\" />\n<br class=\"t-last-br\" />","✓"]
["2,155 kg max. payload 600 mm from implement pivot axis<br class=\"t-last-br\" />","✓"]