{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":1,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":34,"n_cols":2,"rows_kept":34,"cut":false,"hidden":false,"merged":[]}
[]
["Technical Specifications","MAGNUM 400 ROWTRAC"]
["ENGINE"]
["FPT - EU Stage V (Hi-eSCR2)<br class=\"t-last-br\" />","✓"]
["Rated power acc. ECE R120 [kW/hp]<br class=\"t-last-br\" />","291 / 396"]
["Maximum power acc. ECE R120 [kW/hp]<br class=\"t-last-br\" />","320 / 435"]
["Number of cylinder / capacity [cm3]<br class=\"t-last-br\" />","6 / 8,700"]
["Max torque [Nm]<br class=\"t-last-br\" />","1.850 @ 1,400 rpm"]
["Torque rise [%]<br class=\"t-last-br\" />",33]
["<span style=\"background-color: #ffffff; text-align: left; letter-spacing: normal; color: #444444;\">Diesel / AdBlue capacity [litres]</span>","674 / 99"]
["TRANSMISSION"]
["PowerDrive - 21x5 gears, Full-Powershift transmission, 40 kph ECO<br class=\"t-last-br\" />","✓"]
["APM (Automatic Productivity Management)<br class=\"t-last-br\" />","✓"]
["Automatic mode field &amp; road<br class=\"t-last-br\" />","✓"]
["HYDRAULICS"]
["Axial piston pump with load sensing<br class=\"t-last-br\" />","221 l/min "]
["Electrical rear remotes, Power Beyond, <span style=\"background-color: #ffffff; text-align: start; letter-spacing: normal; color: #000000;\">external fender controls</span><br class=\"t-last-br\" />\n<br class=\"t-last-br\" />",6]
["Front linkage, advanced joystick<br class=\"t-last-br\" />\n<br class=\"t-last-br\" />","✓"]
["PTO"]
["1,000 @ 1,803 rpm, external control 540E/1,000 @ 1,592/1.803 rpm<br class=\"t-last-br\" />","✓"]
["REAR LINKAGE"]
["EDC with dynamic ride control - max. lift capacity 10,929 kg<br class=\"t-last-br\" />","✓"]
["TRACKS REAR"]
["Gauge: 2,230 mm, rubber track: 762 mm<br class=\"t-last-br\" />","✓"]
["Automatic, hydraulic clamping system<br class=\"t-last-br\" />","✓"]
["Form-fitting driven &amp; self-cleaning<br class=\"t-last-br\" />","✓"]
["CONFIGURATION"]
["AFS Pro 1200 monitor with ISOBUS Cl. III<br class=\"t-last-br\" />","✓"]
["Semi-active suspended Luxury Performance Cab<br class=\"t-last-br\" />","✓"]
["360&deg; LED work lights, tire pressure sensor system<br class=\"t-last-br\" />","✓"]
["HMC II &amp; configurable remotes<br class=\"t-last-br\" />","✓"]
["Auto guidance System AccuGuide &amp; AccuTurn Pro (automatic turning)<br class=\"t-last-br\" />","✓"]
["AFS Connect - Advanced Telematics + Adaptive Steering Control (Fast steering)<br class=\"t-last-br\" />","✓"]
["Automatic steering brake<br class=\"t-last-br\" />","✓"]