{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":1,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":36,"n_cols":2,"rows_kept":36,"cut":false,"hidden":false,"merged":[]}
[]
["Technical Specifications","AXIAL-FLOW 9260​"]
["ENGINE"]
["FPT &ndash; Cursor 16 - EU Stage V<br class=\"t-last-br\" />","✓"]
["Maximum power acc. ECE R120 [kW/hp]<br class=\"t-last-br\" />","466 / 634"]
["Number of cylinder / capacity [cm3]<br class=\"t-last-br\" />","6 / 15,900"]
["<span style=\"background-color: #ffffff; text-align: left; letter-spacing: normal; color: #444444;\">Diesel / AdBlue capacity [litres]</span>","1,200 / 166"]
["THRESHING / SEPARATING"]
["Rotor drive type<br class=\"t-last-br\" />","Gearbox and shaft - variable speed Power Plus Drive with reverser"]
["Rotor speed range<br class=\"t-last-br\" />","220 - 1,180 rpm (3 ranges)"]
["Rotor diameter and length<br class=\"t-last-br\" />","762 mm / 2,638 mm"]
["Total separation area<br class=\"t-last-br\" />","2.98 m2​"]
["Threshing / separating modules wrap angle<br class=\"t-last-br\" />","180° / 180°"]
["Number of threshing / separation modules<br class=\"t-last-br\" />","2026-02-02"]
["CLEANING SYSTEM"]
["Cascade sieve standard<br class=\"t-last-br\" />","✓"]
["Cleaning shoe width<br class=\"t-last-br\" />","1.58 m"]
["Levelling capability<br class=\"t-last-br\" />","12.1 %"]
["Total sieve area under wind control<br class=\"t-last-br\" />","6.5 m2​ ​"]
["RETURN SYSTEM"]
["Triple impeller tailings processor directly to grain pan<br class=\"t-last-br\" />","✓"]
["GRAIN TANK / UNLOADING"]
["In-cab control of grain tank covers<br class=\"t-last-br\" />","✓"]
["Grain tank capacity<br class=\"t-last-br\" />"," 14,400 l​"]
["Standard / High capacity unload rate<br class=\"t-last-br\" />","113 l/s / 159 l/s"]
["Unloading auger effective length, measured from middle of combine to tip of unloading auger Standard<br class=\"t-last-br\" />","6.7 or 7.6 m​"]
["High capacity options<br class=\"t-last-br\" />","7.2 or 8.8 m​"]
["STRAW CHOPPER & SPREADER"]
["Integral fixed knife chopper with X-tra chopping system<br class=\"t-last-br\" />","option"]
["Number of knives: chopper / counter bar X-tra chopping system<br class=\"t-last-br\" />","Integral pre-chopper with 40/40 knives plus hood mount chopper with 96 knives​"]
["Spreader type<br class=\"t-last-br\" />","Integral chopper: Vertical, twin disc hydraulically driven, in cab speed adjustable​"]
["X-tra chopping system<br class=\"t-last-br\" />","Independent spread boards"]
["AUTOMATION"]
["AFS Harvest Command<sup>TM</sup><br class=\"t-last-br\" />","✓"]
["Harvesting strategies<br class=\"t-last-br\" />",4]
["Patented sieve pressure sensors and multi spectrum grain quality camera<br class=\"t-last-br\" />","✓"]