{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":1,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":64,"n_cols":4,"rows_kept":64,"cut":false,"hidden":false,"merged":[]}
[]
[null,"Patriot 4450","Patriot 4350","Patriot 3250"]
["Solution System"]
["Min Solution System Tank gallon (US)",1600,1200,800]
["Max Solution System Tank gallon (US)",1600,1200,1000]
["Tank Material ","Stainless Steel","Stainless Steel","Stainless steel"]
["Fill Connection in",3,3,3]
["Other Tanks And Containers"]
["Rinse Tank gallon (US)",160,140,100]
["Hand Wash Tank gallon (US)",4.5,4.5,4.5]
["Foam Marker Tank gallon (US)",3,3,3]
["Fuel Tank gallon (US)",150,150,150]
["DEF Tank gallon (US)",21.5,21.5,21.5]
["Boom"]
["Boom Location ","Rear","Rear","Rear"]
["Boom Width - Option 1 ","60/90ft (18.3/27.4 m)","60/90ft (18.3/27.4 m)","60/90ft (18.3/27.4 m)"]
["Boom Width - Option 2 ","60/90/120ft (18.3/27.4/36.5 m)","60/90/120ft (18.3/27.4/36.5 m)","60/90/120ft (18.3/27.4/36.5 m)"]
["Boom Width - Option 3 ","69/135ft (21/41.1 m)","69/135ft (21/41.1 m)","69/135ft (21/41.1 m)"]
["Min Ground Height Adjustment in",24,24,24]
["Max Ground Height Adjustment in",84,84,84]
["Nozzle Spacing - In (cm) ","20 (50.8)  or 30 (76.2)","20 (50.8)  or 30 (76.2)","20 (50.8)  or 30 (76.2)"]
["Engine"]
["Position ","Rear","Rear","Rear"]
["Make ","Case IH FPT","Case IH FPT","Case IH FPT"]
["Power hp",390,335,285]
["Peak Torque lbf/ft",1258,1143,856]
["Peak Power hp",415,374,309]
["Number Of Cylinders ",6,6,6]
["Displacement in³",531,531,409]
["Alternator A",null,null,175]
["Drive Train"]
["Description ","Hydrostatic","Hydrostatic","Hydrostatic"]
["Number Of Speed Ranges ","Infinitely variable","Infinitely variable","Infinitely variable"]
["Max Travel Speed mph",37,37,32]
["Drive ","Full-time 4WD","Full-time 4WD","Full-time 4WD"]
["Primary Service Brake ","Drive system dynamic braking","Drive system dynamic braking","Drive system dynamic braking"]
["Secondary Service Brake ","All four wheels, pedal activated","All four wheels, pedal activated","All four wheels, pedal activated"]
["Parking Brake ","Spring-applied hydraulic released wet disc, all wheels","Spring-applied hydraulic released wet disc, all wheels","Spring-applied hydraulic released wet disc, all wheels"]
["Cab"]
["Cab Position ","Ahead of front axle","Ahead of front axle","Ahead of front axle"]
["Cab Glass Area ft²",88.1,88.1,88.1]
["Operator Seat Description ","Air suspension; 30degree swivel","Air suspension; 30degree swivel","Air suspension; 30degree swivel"]
["Sprayer Control ","AIM Command FLEX, using Case IH AFS Pro 700 or Case IH Viper 4+","AIM Command FLEX, using Case IH AFS Pro 700 or Case IH Viper 4+","AIM Command FLEX, using Case IH AFS Pro 700 or Case IH Viper 4+"]
["Chassis"]
["Crop Clearance ft-in","4ft 8in","4ft 5in","4ft 5in"]
["Min Wheel Track Spacing ft-in","9ft 10in","9ft 10in","9ft 10in"]
["Max Wheel Track Spacing ft-in","13ft 4in","13ft 4in","13ft 4in"]
["Wheel Track Adjustment Method ","Hydraulic, from cab","Hydraulic, from cab","Hydraulic, from cab"]
["Wheelbase ft-in","13ft 4in","13ft 4in","12ft 6in"]
["Steering System ","2WS, Hydraulic","2WS, Hydraulic","2WS, Hydraulic"]
["Suspension Description ","Air spring and shock absorber","Air spring and shock absorber","Air spring and shock absorber"]
["Suspension Travel in",8,8,8]
["Tires"]
["Standard Row-crop Tire ","VF 380/105 R50","IF 320/90 R46","IF 320/90 R46"]
["Optional Row-crop Tire 1 ","VF 420/95 R50","VF 380/90 R46","380/90 R46"]
["Optional Row-crop Tire 2 ","VF 480/80 R50","LSW 480/70 R46","VF 380/90 R46"]
["Overall Dimensions, Boom Folded"]
["Length ft-in","30ft 1in","30ft 5in","29ft 7in"]
["Height ft-in","12ft 11in","12ft 1in","11ft 9in"]
["Width - Wheels Retracted ft-in","12ft 7in","12ft 7in","12ft"]
["Dry Weight"]
["Weight W/ Shortest Boom lb",null,null,28732]
["Weight W/ Intermediate Boom lb",33720,32400]
["Weight W/ Widest Boom lb",null,null,30340]