{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":1,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":38,"n_cols":5,"rows_kept":38,"cut":false,"hidden":false,"merged":[]}
[]
[null,"True-Tandem 335VT","True-Tandem 335 Barracuda","True-Tandem 335 VT (large)","VT-Flex 435 Vertical Tillage Tool"]
["Configuration"]
["Fore-aft Configuration ","Blade-Blade-Rolling reel","Blade-Blade-Rolling reel","Blade-Blade-Rolling reel","Blade-Blade-Basket"]
["Primary Blade Type ","Wave blade","Serrated, modified wave turbo blade","Wave blade","Coulter"]
["Manufacturer's Description Of Blades ","Earth Metal VT Wave Blade","Earth Metal Barracuda Blade","Earth Metal VT Wave Blade","Earth Metal VT Wave Blade"]
["Dimensions And Weights"]
["Min Working Width ft-in","22ft 2in","22ft 5in","42ft 5in","11ft"]
["Max Working Width ft-in","34ft 1in","34ft 3in","47ft 2in","34ft"]
["Min Transport Width ft-in","14ft 6in","14ft 6in","18ft 6in","13ft"]
["Max Transport Width ft-in","18ft","18ft","18ft 6in","17ft 10in"]
["Min Transport Height ft-in","10ft 5in","10ft 5in","13ft 2in","9ft"]
["Max Transport Height ft-in","13ft 7in","13ft 7in","13ft 2in","13ft 10in"]
["Min Weight lb",15377,15600,28000]
["Max Weight lb",21588,21900,32815]
["Sizes Available ",5,5,2,7]
["Blades"]
["Blade Diameter in",20,22,20,20]
["Blade Spacing in",7.5,7.5,null,7.5]
["Blade Edge Profile ","Wave pattern, can be sharpened","Chisel-tip blade serrations","Wave pattern, can be sharpened","Wave"]
["Blade Concavity ","Slight concavity","Shallow concavity","Slight concavity","Shallow concavity"]
["Blade Mounting And Angles"]
["Blade Mounting ","Gangs","Gangs","Gangs","Gangs"]
["Front Angle Of Gang Or Blades - ° ",18,18,18,12]
["Rear Angle Of Gang Or Blades - ° ",18,18,18]
["Rolling Basket, Reel Or Chopper"]
["Description ","Double Edge Rolling Reel","Double Edge Rolling Reel","Rolling Reel","Basket"]
["Rolling Diameter in",null,14,null,14]
["Bars Or Blades On Circumference ","Formed double edge on each bar","Formed double edge on each bar","Flat or round bars, spiral pattern","Bars"]
["Harrow"]
["Harrow Tool ","Coil tine optional","Coil tine optional","Coil tine optional"]
["Harrow Gangs ","3-bar optional, for rice areas only","3-bar optional, for rice areas only","3-bar optional, for rice areas only"]
["Tires"]
["Transport Tire, Largest Size ","12.5x15 FI up to 380/60 R16.5","12.5x15 FI up to 380/60 R16.5","16.5Lx16.1 FI up to 440/55 R18","340/55 - 16"]
["Wing Tire, Largest Size ","11Lx15, 8 ply","11Lx15, 8 ply","12.5Lx15 FI"]
["Tractor Power Recommendations"]
["Power Per Width Of Cut - Low hp/ft",5,10,5.95,5.9]
["Power Per Width Of Cut - High hp/ft",10,15,10,11.17]