{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":1,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":127,"n_cols":13,"rows_kept":127,"cut":false,"hidden":false,"merged":[]}
[]
[null,"Magnum 200","Magnum 220","Magnum 240","Magnum 265","Magnum 295","Magnum 325","Magnum 355","Magnum 385","Magnum 405","Magnum 340 Rowtrac","Magnum 380 Rowtrac","Magnum 400 Rowtrac"]
["Description"]
["Classification Horsepower ","200","220","240",{"$nulls":6},"340","380"]
["Drive Type ","Wheeled Tractor","Wheeled Tractor","Wheeled Tractor",{"$nulls":6},"Tracked Tractor - 2 Tracks","Tracked Tractor - 4 Tracks"]
["Drive Configuration ","4WD","4WD","4WD",{"$nulls":6},"2 Wheel / 2 Tracks"]
["Application ",{"$nulls":9},"Row Crop"]
["Engine Performance"]
["Rated Engine Power hp","200","220","240",{"$nulls":6},"340","380"]
["Max Power (No Boost) hp","220","240","260",{"$nulls":6},"375","415"]
["Max Power (Boost) hp","245","260","270",{"$nulls":6},"410"]
["Power Boost hp","25","20","10",{"$nulls":6},"35","55"]
["Rated Speed rpm","2100","2100","2100",{"$nulls":6},"2000","2000","2000"]
["Rating Standard ","ECE R120","ECE R120","ECE R120",{"$nulls":8},"ECE R210"]
["Fuel Tank gallon (US)","160","160","160",{"$nulls":6},"179","163","179"]
["DEF Tank gallon (US)","17.5","17.5","17.5",{"$nulls":6},"26","26","26"]
["Electric Drivetrain Performance"]
["Motor Performance "]
["Traction Battery "]
["Power Take Off (PTO)"]
["Type ",{"$nulls":9},"Independent","Independent","Independent"]
["Rear PTO "]
["PTO Power hp","170","185","205",{"$nulls":6},"290","315"]
["540rpm "]
["540 Available? ","Yes","Yes","Yes",{"$nulls":6},"Optional","Optional"]
["Engine Speed At 540 rpm","2100","2100","2100"]
["1000rpm "]
["1000 Available? ","Yes","Yes","Yes",{"$nulls":6},"Yes","Yes"]
["Engine Speed At 1000 rpm",{"$nulls":10},"2000"]
["Front PTO "]
["Engine"]
["Details "]
["Make ","FPT","FPT","FPT",{"$nulls":6},"FPT","FPT"]
["Model ",{"$nulls":9},"8.7 L","8.7 L"]
["Cylinders ","6","6","6",{"$nulls":6},"6","6","6"]
["Displacement in³","409","409","409",{"$nulls":6},"531","531","531"]
["Engine Bore in",{"$nulls":9},"4.61","4.61"]
["Engine Stroke in",{"$nulls":9},"5.31","5.31"]
["Block Design ",{"$nulls":9},"Wet liners","Wet liners"]
["Aspiration ","Turbocharger","Turbocharger","Turbocharger",{"$nulls":6},"Turbocharger","Turbocharger","Turbocharger"]
["Fuel System "]
["Description ",{"$nulls":9},"Common Rail","Common Rail","Common Rail"]
["System Control ",{"$nulls":9},"Electronic","Electronic","Electronic"]
["Fuel Injection ",{"$nulls":9},"Direct","Direct","Direct"]
["Emission Treatment "]
["Exhaust Gas Recirculation ",{"$nulls":9},"No","No","No"]
["Cleanup Catalyst (CUC) ",{"$nulls":9},"Yes","Yes","Yes"]
["Diesel Oxidation Catalyst ",{"$nulls":9},"Yes","Yes","Yes"]
["Diesel Particulate Filter ",{"$nulls":9},"No","No","No"]
["Selective Catalytic Reduction (SCR) ","Yes","Yes","Yes",{"$nulls":6},"Yes","Yes","Yes"]
["Exhaust Orientation ","Vertical","Vertical","Vertical",{"$nulls":6},"Vertical","Vertical","Vertical"]
["Electrical System"]
["System Rating V",{"$nulls":9},"12","12"]
["Alternator "]
["Voltage V","12","12","12",{"$nulls":6},"12","12","12"]
["Rating A","200","200","200",{"$nulls":6},"200","200","240"]
["Engine Battery "]
["Transmission Configuration"]
["Description ","PowerDrive","PowerDrive","CVXDrive",{"$nulls":6},"PowerDrive","CVXDrive","PowerDrive FPS 21x5"]
["Type ","Powershift","Powershift","Continuously Variable Transmission (CVT)",{"$nulls":6},"Powershift","Continuously Variable Transmission (CVT)"]
["Forward Speeds ","19","19",{"$nulls":7},"18","4"]
["Reverse Speeds ",{"$nulls":9},"4","2"]
["Max Speed Forward - mph (kph) ",{"$nulls":10},"25 (40) most track widths MY2019"]
["Max Speed mph","25","25","25",{"$nulls":6},"25","25","25"]
["Creeper Range ",{"$nulls":9},"Optional","Standard","No"]
["Shuttle Available ",{"$nulls":9},"Yes","Yes","Yes"]
["Optional Transmission 1"]
["Description ","PowerDrive","PowerDrive","CVXDrive",{"$nulls":6},"CVXDrive"]
["Type ","Powershift","Powershift","Continuously Variable Transmission (CVT)",{"$nulls":6},"Continuously Variable Transmission (CVT)"]
["Forward Speeds ","19","19",{"$nulls":7},"4"]
["Reverse Speeds ",{"$nulls":9},"2"]
["Max Speed mph","30","30","30",{"$nulls":6},"25"]
["Optional Transmission 2"]
["Description ","CVXDrive","CVXDrive"]
["Type ","Continuously Variable Transmission (CVT)","Continuously Variable Transmission (CVT)"]
["Max Speed mph","25","25"]
["Wheel Or Track Configuration"]
["Drive Configuration ","4WD","4WD","4WD",{"$nulls":6},"2 Rear Tracks + 2 MFD Front Tires","2 Rear Tracks + 2 MFD Front Tires","2 Rear Tracks + 2 MFD Front Tires"]
["Steering Configuration ","Front Steer","Front Steer","Front Steer",{"$nulls":6},"Front Steer","Front Steer","Front Steer"]
["Hydraulic System"]
["System Type ","Pressure Flow Compensated (PFC)","Pressure Flow Compensated (PFC)","Pressure Flow Compensated (PFC)",{"$nulls":6},"Pressure Flow Compensated (PFC)","Pressure Flow Compensated (PFC)","Pressure Flow Compensated (PFC)"]
["Implements "]
["Pump Type ",{"$nulls":9},"Variable Displacement","Variable Displacement","Variable displacement"]
["Standard Pump Flow gallon (US)/min","41","41","41",{"$nulls":6},"44","44"]
["Optional Pump Flow gallon (US)/min","43","43","43",{"$nulls":6},"59","59"]
["Remote Valves ","3","3","3",{"$nulls":6},"4 std; 5 or 6 opt","4 std; 5 or 6 opt"]
["Steering "]
["3-Point Hitch"]
["Features "]
["3-Point Hitch Category ","Category 3/3N","Category 3/3N","Category 3/3N",{"$nulls":6},"Category 4/3","Category 4/3"]
["Optional Hitch Category ",{"$nulls":9},"Category 3N w/ Quick-Coupler","Category 3N w/ Quick-Coupler","Category 3"]
["Draft Sensing Or Lift Control ",{"$nulls":9},"Electronic position and/or draft control","Electronic position and/or draft control","Electronic position and/or draft control"]
["Draft Link Ends Telescopic ",{"$nulls":9},"Adjustable quick coupler","Adjustable quick coupler","Adjustable quick coupler"]
["Lift Capacity "]
["Standard Capacity 24 Inches Behind Pin lb",{"$nulls":10},"19900"]
["Optional Lift Capacity 24 Inches Behind Pin - lb (kg) ",{"$nulls":10},"No 3N setting w/quick coupler"]
["Standard Capacity At Pin lb",{"$nulls":9},"17500"]
["Max Lift Capacity lb","13600","13600","13600",{"$nulls":7},"19900"]
["Dimensions"]
["Wheelbase in","118","118","118",{"$nulls":6},"124","124"]
["Length in",{"$nulls":9},"249","249"]
["Height Over Cab in",{"$nulls":9},"136","136"]
["Overall Width, With Standard Wheels Or Tracks - In (mm) ",{"$nulls":10},"93 (2362) min.; 182 (4623) max."]
["Overall Width in",{"$nulls":9},"93"]
["Weight"]
["Unladen Weight lb",{"$nulls":10},"36000"]
["Weight lb","21500","21500","21500",{"$nulls":6},"36000","0","36000"]
["Weight Without Ballast lb",{"$nulls":9},"36000","36000","36000"]
["Tire / Track Size"]
["Front Tire Size, 2WD ",{"$nulls":10},"No 2WD"]
["Front Tire Size ",{"$nulls":9},"IF 420/85 R38 R1W","IF 420/85 R38 R1W","IF 420/85 R38 R1W"]
["Rear Tire Size ",{"$nulls":9},"Track (MY2019) 16, 18, 21, 24, 30 (406, 457, 553, 610, 762)","Track (MY2019) 16, 18, 21, 24, 30 (406, 457, 553, 610, 762)","Rubber Track 18 (457) std; 16, 21, 24, 30 opt"]
["Tracks "]
["Cooling System"]
["Fan Drive Type ",{"$nulls":9},"BorgWarner Visctronic","BorgWarner Visctronic","Viscous"]
["Rear Axle Assembly"]
["Final Drive ",{"$nulls":9},"Planetary - Inboard  ","Planetary - Inboard  ","Planetary - Inboard  "]
["Axle Output ",{"$nulls":9},"Flange w/ drive sprocket","Flange w/ drive sprocket","Flange w/drive sprocket"]
["Axle Bar Diameter - in (mm) ",{"$nulls":9},"No bar axle","No bar axle"]
["Front Axle"]
["Suspended Front Axle Available ",{"$nulls":9},"Optional","Optional","Optional"]
["Brakes"]
["Service Brake ",{"$nulls":9},"Wet Disc","Wet Disc","Wet Disc"]
["Drawbar"]
["Drawbar Description ",{"$nulls":9},"Category 4, Adjustable","Category 4, Adjustable","Category 4, Adjustable"]
["PTO Performance"]
["PTO Speeds - Rpm ",{"$nulls":10},"1000 std; 540 / 1000 opt"]