{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":1,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":61,"n_cols":22,"rows_kept":61,"cut":false,"hidden":false,"merged":[]}
[]
[null,"Puma 150","Puma 150 CVT","Puma 165","Puma 165 CVT","Puma 175","Puma 185","Puma 185 CVT","Puma 200","Puma 200 CVT (2011)","Puma 220","Puma 220 CVT","Puma 240","Puma 185 CVT (2011)","Puma 185 Powershift (2011)","Puma 200 PS or CVT (2014)","Puma 200 PS (2011)","Puma 240 CVT","Puma 125","Puma 130","Puma 170","Puma 215"]
["Description"]
["Classification Horsepower ",150,150,165,165,180,185,185,200,null,null,220,240,185,185,240,200,240,125,130,170]
["Drive Type ","Wheeled Tractor","Wheeled Tractor","Wheeled Tractor","Wheeled Tractor","Wheeled Tractor","Wheeled Tractor","Wheeled Tractor","Wheeled Tractor",null,null,"Wheeled Tractor","Wheeled Tractor","Wheeled Tractor","Wheeled Tractor",null,"Wheeled Tractor","Wheeled Tractor","Wheeled Tractor","Wheeled Tractor","Wheeled Tractor"]
["Drive Configuration ","4WD","4WD","4WD","4WD","4WD","4WD","4WD","4WD",null,null,"4WD",null,"4WD","4WD",null,"4WD","4WD","4WD","4WD","4WD"]
["Application ","Row Crop","Row Crop","Row Crop","Row Crop"]
["Engine Performance"]
["Rated Engine Power hp",150,150,165,165,180,180,180,200,null,null,220,"240  [177]",185,185,"240  [177]",200,240,125,131,167]
["Max Power (No Boost) hp",165,165,180,180,null,200,200,220,null,null,240,"270  [199]",234,234,"270  [199]",250,260,148,171,218]
["Max Torque lbf/ft"]
["Power Take Off (PTO)"]
["Rear PTO "]
["PTO Power hp",125,125,140,140,150,150,150,170,null,null,190,"210  [157]",150,150,"210  [157]",165,210,105,105,140]
["540rpm "]
["540 Available? ","Yes","Yes","Yes","Yes","Yes","Yes","Yes","Yes",null,null,"Yes","Yes","Yes","Yes","Yes","Yes","Yes","Yes","Yes","Yes"]
["540E Available? ",{"$nulls":4},"Yes","Optional",null,"Optional",null,null,"Optional","Optional",null,null,"Optional",null,"Optional"]
["1000rpm "]
["1000 Available? ","Yes","Yes","Yes","Yes","Yes","Yes","Yes","Yes",null,null,"Yes",null,"Yes","Yes",null,"Yes","Yes","Yes","Yes","Yes"]
["1000E Available? ",{"$nulls":4},"Optional","Optional","Optional","Optional",null,null,"Optional","Optional","Yes","Yes","Optional","Yes","Optional",null,null,"Yes"]
["Front PTO "]
["Engine"]
["Make ","FPT","FPT","FPT","FPT","FPT","FPT","FPT","FPT",null,null,"FPT","Case IH FPT","FPT","FPT","Case IH FPT","FPT","FPT","FPT","FPT","FPT"]
["Model ",{"$nulls":11},"6.7 L","6.7 L","6.7 L","6.7 L","6.7 L",null,"NEF 667TA","6.7 L","6.7 L"]
["Electrical System"]
["Alternator "]
["Transmission Configuration"]
["Type ","Powershift","Continuously Variable Transmission (CVT)","Powershift","Continuously Variable Transmission (CVT)","Continuously Variable Transmission (CVT)","Powershift","Continuously Variable Transmission (CVT)","Powershift",null,null,"Continuously Variable Transmission (CVT)","CVT","Continuously Variable Transmission (CVT)","Powershift","CVT","Powershift","Continuously Variable Transmission (CVT)","Powershift","Powershift","Powershift"]
["Forward Speeds ",18,null,18,null,null,18,null,18,null,null,null,4,4,18,4,18,null,18,18,18]
["Reverse Speeds ",6,null,6,null,null,6,null,6,null,null,null,2,4,6,4,6,null,6,6,6]
["Max Speed Forward - mph (kph) ",{"$nulls":11},"25 or 31 (40 or 50)"]
["Hydraulic System"]
["Standard Pump Flow gallon (US)/min",29,37,29,37,37,31.7,39.6,31.7,null,null,39.6,"39.6  [150]",32,32,"39.6  [150]",32,39.6,26.5,26.5,32]
["Standard Pump Pressure psi",{"$nulls":4},3046]
["Remote Valves ","3 std; 4 or 5 opt","3 std; up to 5 total","3 std; 4 or 5 opt",null,4,"3 std; 4 or 5 opt",null,"3 std; 4 or 5 opt",null,null,null,"3 std; 4 or 5 opt","3 std; 4 or 5 opt","3 std; 4 or 5 opt","3 std; 4 or 5 opt","3 std; 4 or 5 opt",null,2,"2 std; 3 or 4 opt","3 std; 4 or 5 opt"]
["3-Point Hitch"]
["3-Point Hitch Category ","Category 2","Category 2","Category 2","Category 2","Category 2/3","Category 2/3N","Category 2/3N","Category 2/3N",null,null,"Category 2/3N","Category 2/3","Category 2/3N","Category 2/3N","Category 2/3","Category 2/3N","Category 2/3N","Category 2/3N","Category 2","Category 2/3N"]
["Standard Capacity 24 Inches Behind Pin lb",{"$nulls":4},14586,{"$nulls":6},"9450  [4286]",10200,10200,"9450  [4286]",10200,null,7900,7900,10200]
["Standard Capacity At Pin lb",11821,12965,11821,11821,18204]
["Max Lift Capacity lb",19368,null,null,null,18204,9450,9450,9450,null,null,9450,{"$nulls":5},9450]
["Dimensions"]
["Wheelbase in",107.6,107.6,107.6,107.6,108,113.6,113.6,113.6,null,null,113.6,"113.6  [2885]",113.6,113.6,"113.6  [2885]",113.6,113.6,107.8,107.8,113.6]
["Length in",{"$nulls":4},206,{"$nulls":12},179.5,179.5]
["Height Over Cab in",124.2,null,124.2,null,119,{"$nulls":12},118.3,118.3]
["Height Over ROPS in"]
["Overall Width in",{"$nulls":4},81,112,null,112,{"$nulls":6},"112  [2845]"]
["Tire / Track Size"]
["Tracks "]
["Weight"]
["Unladen Weight lb"]
["Weight, Total Allowable lb",{"$nulls":4},25353,{"$nulls":6},"28660  [13000]",28660,28660,"28660  [13000]",28660,null,23149,23149,28660]
["Weight, Total Allowable To 40km/h lb",{"$nulls":4},25353]
["Weight, Total Allowable To 50km/h lb",{"$nulls":4},25353]
["Weight, Total Allowable To 60km/h lb"]
["Electric Drivetrain Performance"]
["Type "]
["Phase "]
["Power hp"]
["Battery Type "]
["Voltage V"]
["Capacity Ah"]