{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":1,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":38,"n_cols":9,"rows_kept":38,"cut":false,"hidden":false,"merged":[]}
[]
[null,"Steiger 785","Steiger 715","Steiger 645","Steiger 595","Steiger 555","Steiger 525","Steiger 475","Steiger 425"]
["Description"]
["Classification Horsepower ","785","715","645","595","555","525","475","425"]
["Engine Performance"]
["Rated Engine Power ","785","715","645","595","555","525","475","425"]
["Max Power (HP) ","853","778","699","656","614","578","522","467"]
["PTO HP ","537","537","537","537","537","516","462","409"]
["Peak Torque (Nm) (1400 eRPM) ","3684","3356","3061","2877","2681","2456","2222","1989"]
["Tank Capacity (Litres/Wheeled Steiger) ","-",null,"1722","1722","1722","1170","1170","1170"]
["Tank Capacity (Litres/Rowtrac) ","-",{"$nulls":4},"1287","1287","1287"]
["Tank Capacity (Litres/Quadtrac) ","1968","1968","1779","1779","1779","1779","1779"]
["Power Take Off (PTO)"]
["1000 Available? ","Optional","Optional","Optional","Optional","Optional","Optional","Optional","Optional"]
["Engine"]
["Engine Make ","FPT","FPT","FPT","FPT","FPT","FPT","FPT","FPT"]
["Engine Model ","Cursor 16 TST","Cursor 16 TST","Cursor 13 TST","Cursor 13 TST","Cursor 13 TST","Cursor 13 EVGT","Cursor 13 EVGT","Cursor 13 EVGT"]
["Displacement ","15.9L","15.9L","12.9L","12.9L","12.9L","12.9L","12.9L","12.9L"]
["Transmission Configuration"]
["Transmission Type ","Powershift","Powershift","Powershift","Powershift","Powershift","Powershift","Powershift","Powershift"]
["Number Of Forward Speeds ","16","16","16","16","16","16","16","16"]
["Max Speed Forward (KPH) ","40","40","40","40","40","40","40","40"]
["Hydraulic System"]
["Total Implement Pump Flow (L/M) ","216","216","216","216","216","216","216","216"]
["Twin Pumps (Optional) Flow (L/M) ","427","427","427","427","427","427","427","427"]
["3 Point Hitch"]
["3 Point Hitch Category ","Category 4N","Category 4N","Category 4N","Category 4N","Category 4N","Category 4N","Category 4N","Category 4N"]
["Wheeled (Kg) ","-",null,"10319","10319","10319","9071","9071","9071"]
["Rowtrac (Kg) ","-",{"$nulls":4},"9071","9071","9071"]
["Quadtrac (Kg) ","10092","10092","10092","10092","10092","10092","10092"]
["Dimensions"]
["Wheelbase (mm) (Wheeled) ","-",null,"3912","3912","3912","3759","3759","3759"]
["Wheelbase (mm) (Rowtrac) ","-",{"$nulls":4},"4063","4063","4063"]
["Wheelbase (mm) (Quadtrac) ","3912","3912","3912","3912","3912","3912","3912"]
["Max Weight"]
["Weight, Total Allowable (kg) (Wheeled) ","-",null,"30390","30390","27215","25401","25401","25401"]
["Weight, Total Allowable (kg) (Rowtrac) ","-",{"$nulls":4},"27215","27215","27215"]
["Weight, Total Allowable (kg) (Quadtrac) ","32658","32658","30390","30390","30390","30390","30390","30390"]