{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":1,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":68,"n_cols":7,"rows_kept":68,"cut":false,"hidden":false,"merged":[]}
[]
[null,"Farmall 110 JX","Farmall 100 JX","Farmall 90 JX","Farmall 80 JX","Farmall 75 JX","Farmall 70 JX"]
["Engine"]
["Number of cylinders ",4,4,4,3,4,3]
["Type ","Diesel engine, turbocharged and intercooled","Diesel engine, turbocharged and intercooled","Diesel engine, turbocharged and intercooled","Diesel engine, turbocharged and intercooled","Diesel engine, turbocharged and intercooled","Diesel engine, turbocharged and intercooled"]
["Emission Level ","Tier 3","Tier 3","Tier 3","Tier 3","Tier 3","Tier 3"]
["Capacity (cm³) ","3,908","3,908","3,908","2,930","3,908","2,930"]
["Engine Performance"]
["Maximum engine power with Power Management (hp (kW)) ","-","-","-","-","-","-"]
["Maximum engine power (hp (kW)) ","-","-","-","-","-","-"]
["@ engine speed (rpm) "," "," "," "," "," "," "]
["Rated engine power with Power Management (hp (kW)) ","-","-","-","-","-","-"]
["Rated engine power (hp (kW)) ","110 (81)","98 (73)","88 (66)","80 (60)","75 (56)","65 (49)"]
["Rated engine speed (rpm) ","2,300","2,300","2,500","2,500","2,300","2,300"]
["Maximum torque Power Management (Nm @ rpm) ","-","-","-","-","-","-"]
["Maximum torque (Nm @ rpm) ","430 @ 1400","390 @ 1400","356 @ 1400","320 @ 1400","298 @ 1400","261 @ 1400"]
["Torque rise Standard and Power Management (%) ","-","-","-","-","-","-"]
["Fuel tank capacity diesel / urea (litres) ","110 (-)","110 (-)","110 (-)","110 (-)","110 (-)","110 (-)"]
["Standard Transmission"]
["Transmission Type ","12 x 12 Synchro shuttle transmission","12 x 12 Synchro shuttle transmission","12 x 12 Synchro shuttle transmission","12 x 4 Synchro command transmission","12 x 4 Synchro command transmission","12 x 4 Synchro command transmission"]
["Maximum Speed Forward (kp/h) ",30,30,30,30,30,30]
["Powershuttle ","-","-","-","-","-","-"]
["Creeper ","-","-","-","-","-","-"]
["Optional Transmission 1"]
["Transmission Type ","12x12 Hydraulic transmission  Powershuttle","12x12 Hydraulic transmission  Powershuttle","12x12 Hydraulic transmission  Powershuttle","12 x 12 Synchro shuttle transmission","12 x 12 Synchro shuttle transmission","12 x 12 Synchro shuttle transmission"]
["Maximum Speed Forward (kp/h) ",30,30,30,30,30,30]
["Powershuttle ","Option","Option","Option","Option","-","-"]
["Creeper ","-","-","-","-","-","-"]
["Optional Transmission 2"]
["Transmission Type ","-","-","20x12 Synchro Shuttle™ transmission","12x12 Hydraulic  transmission","-","-"]
["Maximum Speed Forward (km/h) ",30,30,30,30,"-","-"]
["Powershuttle ","-","-","-","Std.","-","-"]
["Creeper "," "," ","Option","-","-","-"]
["Optional Transmission 3"]
["Transmission Type "," "," ","20x12 Synchro Shuttle™ transmission","20x12 Synchro Shuttle™ transmission","20x12 Synchro Shuttle™ transmission","20x12 Synchro Shuttle™ transmission"]
["Maximum Speed Forward (km/h) ","-","-",30,30,30,30]
["Powershuttle ","-","-","-","-","-","-"]
["Creeper "," "," ","Option","Option","Option","Option"]
["Power Take Off"]
["PTO Type ","-","-","-","-","-","-"]
["Speed Standard @ rpm ",540,540,540,540,540,540]
["Speed Optional @ rpm ","540 / 540E or 540 / 1000","540 / 540E or 540 / 1000","540 / 540E or 540 / 1000","540 / 540E or 540 / 1000","540 / 540E or 540 / 1000","540 / 540E or 540 / 1000"]
["Ground drive ","Std.","Std.","Std.","Std.","Std.","Std."]
["Shaft type ","-","-","-","-","-","-"]
["Front PTO and hitch"]
["Speed Standard @ rpm ","-","-","-","-","-","-"]
["Front hitch lift capacity ","-","-","-","-","-","-"]
["Drive and Steering (Driveline)"]
["2WD ","Yes","Yes","Yes","Yes","Yes","Yes"]
["4WD ","Yes","Yes","Yes","Yes","Yes","Yes"]
["Front axle suspension ","-","-","-","-","-","-"]
["Steering angle (°) ","55 (2WD) / 40 (4WD)","55 (2WD) / 40 (4WD)","55 (2WD) / 40 (4WD)","55 (2WD) / 40 (4WD)","55 (2WD) / 40 (4WD)","55 (2WD) / 40 (4WD)"]
["Min.turning radius (m) ","-","-","-","-","-","-"]
["Rear axle diff-lock ","-","-","-","-","-","-"]
["Service Brake Type ","-","-","-","-","-","-"]
["ABS Anti-lock braking system ","-","-","-","-","-","-"]
["Hydraulic System"]
["System Type ","-","-","-","-","-","-"]
["Max. pump flow rate Standard / Option ","40,Jan-51,7","40,Jan-51,7","40,Jan-51,7","40,Jan-51,7","40,Jan-51,7","40,Jan-51,7"]
["System pressure (bar) ","-","-","-","-","-","-"]
["Control type ","Mechanical Draft Control ( MDC)","Mechanical Draft Control ( MDC)","Mechanical Draft Control ( MDC)","Mechanical Draft Control ( MDC)","Mechanical Draft Control ( MDC)","Mechanical Draft Control ( MDC)"]
["Max. lift capacity (kg) ","4,700","4,700","4,700","3,565","3,565","3,000"]
["OECD lift capacity through range @ 610 mm (kg) ","3,450","3,450","3,450","2,700","2,700","2,260"]
["Max. number of rear remotes valves ",3,3,3,3,3,3]
["Max. number of mid mount valves ",2,2,2,2,2,2]
["Remote valve timer control ","-","-","-","-","-","-"]
["Category type ","-","-","-","-","-","-"]
["Slip control ","-","-","-","-","-","-"]