{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":1,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":33,"n_cols":2,"rows_kept":33,"cut":false,"hidden":false,"merged":[]}
[]
["Technical Specifications","QUANTUM 120N"]
["ENGINE"]
["FPT - EU Stage V (UltraCompact Hi-eSCR2)<br class=\"t-last-br\" />","✓"]
["Rated power acc. ECE R120 [kW/hp]<br class=\"t-last-br\" />","88 / 120"]
["Number of cylinder / capacity [cm3]<br class=\"t-last-br\" />","4 / 3,600"]
["Max torque [Nm]<br class=\"t-last-br\" />","518 @ 1,300 rpm"]
["Torque rise [%]<br class=\"t-last-br\" />",42]
["<span style=\"background-color: #ffffff; text-align: left; letter-spacing: normal; color: #444444;\">Diesel / AdBlue capacity [litres]</span>","90 / 11"]
["TRANSMISSION"]
["ActiveDrive 2 - 24x24 gears, 2-speed Powershift, 40 kph<br class=\"t-last-br\" />","✓"]
["Adjustable Powershuttle<br class=\"t-last-br\" />","✓"]
["Power Clutch<br class=\"t-last-br\" />","✓"]
["HYDRAULICS"]
["Open Center pump 80 l/min + 36 l/min steering pump<br class=\"t-last-br\" />","✓"]
["Rear Electro-Hydraulic Remotes + Mid-Mount Remotes<br class=\"t-last-br\" />",4]
["Incl. free return<br class=\"t-last-br\" />\n<br class=\"t-last-br\" />","✓"]
["Optional Rear Power Beyond<br class=\"t-last-br\" />\n<br class=\"t-last-br\" />","✓"]
["PTO"]
["540 / 540E / 1000 @ 1,958 / 1,535 / 2,000 rpm incl. stationary PTO<br class=\"t-last-br\" />","✓"]
["Electro-hydraulic PTO engagment<br class=\"t-last-br\" />","✓"]
["Soft start, external control<br class=\"t-last-br\" />","✓"]
["REAR LINKAGE"]
["EDC - max. lift capacity 2,200 kg, 2 external lift rams<br class=\"t-last-br\" />","✓"]
["Rear fender control<br class=\"t-last-br\" />","✓"]
["CONFIGURATION"]
["Comfort Cab incl. Category Cab 4 filter (Twin filter system)<br class=\"t-last-br\" />","✓"]
["Digital dashboard with Encoder<br class=\"t-last-br\" />","✓"]
["Suspended front axle with 3 suspension modes<br class=\"t-last-br\" />","✓"]
["Priemium Air Seat<br class=\"t-last-br\" />","✓"]
["Full LED Package 8 LED work lights<br class=\"t-last-br\" />","✓"]
["Optional FHPL &amp; FPTO<br class=\"t-last-br\" />\n<br class=\"t-last-br\" />","✓"]
["Total width from 1.05 -2.50 m<br class=\"t-last-br\" />\n<br class=\"t-last-br\" />","✓"]